A/C COMPRESSOR TOOL MOD. REWORK INSTALLER TOOL. Cadillac Cimarron 1985

For 1990-2009 cars

# A/C COMPRESSOR TOOL MOD. REWORK INSTALLER TOOL

#### MODELS AFFECTED: 1984 CIMARRON 1985 DEVILLE AND FLEETWOOD

Kent-Moore tool J-33013, the DA-6 A/C compressor hub and drive plate remover and installer, may damage some DA-6,compressor shafts during hub and drive plate removal. To correct this condition, modify the tool as shown in the figure below.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.