SERVICE BULLETIN UPDATE INFORMATION. Cadillac Cimarron 1983

For 1990-2009 cars

# SERVICE BULLETIN UPDATE INFORMATION

1983 SERVICEMAN BULLETIN UPDATE INFORMATION

The listed Serviceman Bulletins require the following corrections be made to them. Please update your bulletins to include these changes.

Serviceman Bulletin Correction -------- ---------- Bulletin No. T 83-27 Step 3 of service procedure should read: File in Group 7 Number 56 ... using Loctite 290 - not Loctite 240. Date Jan. '83

The heading should read: Bulletin No. T 83-28 Bulletin No. T 83-28 File in Group 7 File in Group 7 Number 57 Number 57 not 5 Date Jan. '83 Date Jan. '83

The heading should read: Bulletin No. 1 83-34 Bulletin No. I 83-34 File in Group 8 File in Group 8 Number 26 Number 26 not 25 Date Feb. '83 Date Feb.'83

The heading should read: Bulletin No. T 83-41 Bulletin No. T 83-41 File in Group 6A File in Group 6A Number 31 Number 31 not 30 Date Feb. '83 Date Feb. '83

Bulletin No. T 83-48 The last sentence on the second page File in Group 6A should read: Number 34 For warranty purposes, use Operation Number Date Mar. '83 T 6073 at .8 hour, not Operation Number K6721.

Bulletin No. 1 83-36 The dimensions in Figures 1,2,5,7 and 9 are File in Group 9 listed in both inches and millimeters. All of Number 13 the dimensions listed in millimeters are Date Feb. '83 correct and should be used. All of the dimensions listed in inches are incorrect and should be disregarded.

Bulletin No. T 82-96 Step 4 of service procedure should read: File in Group 6C Number 45 R43TSX plugs should be installed, not Date Aug. '82 R43TS plugs.

Bulletin No. T 83-60 Step A of service procedure should read: File in Group 6C Number 56 ... reading of parameter (.0.1) not Date April '83 parameter (.0.4).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.