MOTOR VEHICLE REGISTRATION DATA. Cadillac Cimarron 1983

For 1990-2009 cars

# MOTOR VEHICLE REGISTRATION DATA

#### SUBJECT: MOTOR VEHICLE REGISTRATION DATA FOR 1983 CADILLAC MOTORS VEHICLES

1983 CADILLAC MOTOR VEHICLE REGISTRATION DATA

CADILLAC VEHICLE DESCRIPTION - WEIGHTS - WHEELBASE - ENGINE DATA

VIN BODY BODY NO. ENGINE SHIPPING WEIGHT SERIES NAME DESIGNATOR TYPE PASS. CODE KILOGRAMS POUNDS ----------- ---------- ---- ----- ---- ---------- ------

FLEETWOOD 2-DOOR 8 1746.8 3851 BROUGHAM COUPE B-47 COUPE N 1897.4 4183

FLEETWOOD 4-DOOR 8 1766.4 3894 BROUGHAM SEDAN B-69 SEDAN N 1924.6 4243

DEVILLE 2-DOOR 6 8 1723.6 3800 COUPE D-47 COUPE N 1874.8 4133

DEVILLE 4-DOOR 8 1750.0 3858 SEDAN D-69 SEDAN N 1900.6 4190

FLEETWOOD LIMOUSINE F-23 8 2100.1 4630 FLEETWOOD 4-DOOR 9 FORMAL LIMOUSINE F-33 SEDAN 7 2139.6 4717 COMMERCIAL CHASSIS -90 - - 6 - -

ELDORADO COUPE L-57 2-DOOR 6 8 1651.1 3640 COUPE N 1802.6 3974

SEVILLE SEDAN S-69 4-DOOR 6 8 1694.7 3736 SEDAN N 1846.2 4070

CIMARRON SEDAN G-69(STD)* 4-DOOR 5 PP 1165.9 2570 G-69(OPT)** SEDAN 1182.3 2607

VIN BODY WHEELBASE ENGINE CU.IN. SERIES NAME DESIGNATOR MILLMETERS INCHES DISPLACEMENT ----------- ---------- ---------- ------ ------------

FLEETWOOD BROUGHAM COUPE B-47

FLEETWOOD V8-250 CU. IN, DIGITAL BROUGHAM SEDAN B-69 3085 121.5 FUEL INJECTION (DFI),

DEVILLE COUPE D-47

DEVILLE SEDAN D-69

FLEETWOOD LIMOUSINE F-23 V8-368 CU.IN.DIGITAL FLEETWOOD 3670 144.5 FUEL INJECTION (DFE) FORMAL LIMOUSINE F-33 ENGINE AVAILABLE ONLY COMMERCIAL CHASSIS -90 FOR LIMOUSINE.

ELDORADO COUPE L-57 V8-368 CU.IN.4 BARREL 2985 144.0 CARBRETOR ENGINE SEVILLE SEDAN S-69 AVAILABLE ONLY FOR COMMERCIAL CHASSIS.

CIMARRON SEDAN G-69(STD)* L-4 121 CU.IN ELECTRONIC G-69(OPT)** 2571 101.2 FUEL INJECTION (EFI)

*Manual Transmission * Automatic Transmission

All weights include automatic transmission, (manual transmission on Cimarron) power steering, power brakes, and air conditioning which are standard on all vehicles. Weights estimated at time of publication. Production weights may vary slightly. Please note: taxable horsepower is 46.2 for the 368 cu.in. engine, 52.7 for the 350 cu.in. engine, 19.6 for the 121 cu.in. engine, and 38.4 for the 250 cu.in. engine. See engine codes below.

ENGINE SPECIFICATIONS

Displacement Cyliner Net Horsepower Fuel Engine Cu.In. Liters Arrangement (SAE J-245) System Code ------ ------ ----------- ----------- ------ ----

250 4.1 V-8 Digital Fuel Digital 8 Injection 101 Fuel (KW) 135 HP Injection

121 2.0 L-4 Electronic Fuel Electronic P Injection 66 Fuel (KW) 88HP Injection

350 5.7 V-8 Diesel 78 Diesel N (KW) 105 HP

368 6.0 V-8 Digital Fuel Digital 9 Injection 105 Fuel (KW) 140 HP Injection

368 6.0 V-8 Carbureted Carburetor 6 112 (KW)150 HP

Displacement Cyliner Bore and Stroke Cu.In. Liters Arrangement Millimeters Inches ------ ------ ----------- ------------ -------

250 4.1 V-8 88.0x84.0 3.46 x 3.31

121 2.0 L-4 89.0x80.0 3.50x3.15

350 5.7 V-8 103.0x86.0 4.057x3.385

368 6.0 V-8 96.5x103.1 3.800x4.060

368 6.0 V-8 96.5x103.1 3.800x4.060

CADILLAC VEHICLE IDENTIFICATION NUMBER INFORMATION

Each 1983 Cadillac automobile or commercial chassis carries a 17-digit vehicle identification number used for license and insurance identification and in general reference to the automobile. The number is located on a plate riveted to the windshield lower frame at the driver's side of the car where it is visible through the windshield. The 1983 Cadillac Vehicle Identifiation Number is decoded as follows:

1G6 = Make "1G6" denotes Cadillac "IGE"denotes Cadillac imcomplete vehicle

A = Restraint System or GVWR/.Brake System Code A-Non Passive Restraint E-6001 lb. to 7000 lb. GVWR range

D=Carline and series

69= Body Type

8 = Engine Code 8 denotes 250 cu.in.with digital fuel injection 4.1 liters N denotes 350 cu.in. diesel 5.7 liters 9 denotes 368 cu.in. with digital fuel injection 6.0 liters 6 denotes 368 cu.in. with carburetor 6.0 liters P denotes 121 cu.in. with electronic fuel injection 2.0 liters

X=Check Digit

D = Model Year (D-1983)

9 = Assembly plant 9 - Detroit, Michigan (C&D Series) E - Linden, New Jersey (E&K Series) J - Janesville, Wisconsin (J Series)

100001 = Production Sequence Number 10001 C & D - Detroit 800001 K - Linden 600001 E - Linden 400001 J - Janesville

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.