CLUSTER INTENSITY MAY BE TOO DIM W/HEADLIGHTS ON. Cadillac Commercial Chassis 1994

For 1990-2009 cars

# CLUSTER INTENSITY MAY BE TOO DIM W/HEADLIGHTS ON

---------------------------------------------------------------------- REVISION 01/04/94

#### BULLETIN REVISED TO UPDATE WARRANTY INFORMATION ADDING TROUBLE CODE.

#### SUBJECT: CLUSTER INTENSITY MAY BE TOO DIM WITH HEADLIGHTS ON IN DAYLIGHT (EXCHANGE CLUSTER)

#### MODELS: 1993-94 CADILLAC FLEETWOOD BROUGHAM

#### CONDITION:

SOME CUSTOMERS MAY COMMENT THAT THE INSTRUMENT PANEL DISPLAY IS TOO DIM WHEN THE HEADLIGHTS ARE TURNED ON DURING DAYLIGHT HOURS.

#### CORRECTION:

A NEW DIMMER INTEGRATED CIRCUIT IS NOW AVAILABLE AT THE CLUSTER REPAIR CENTERS. PLEASE SEND THE CLUSTER IN FOR REPAIR AND REFERENCE THE ABOVE CONDITION. THIS CHANGE WILL BE MADE IN PRODUCTION IN MID-1994.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE: LABOR OPERATION: N4180 USE TROUBLE CODE 92 USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1993 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.