SMU - SEC. 3 - LOWER BALL JOINT REMOVAL TOOL UPDATE. Cadillac Concours 1997

For 1990-2009 cars

# SMU - SEC. 3 - LOWER BALL JOINT REMOVAL TOOL UPDATE

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 3 - LOWER BALL JOINT REMOVAL TOOL UPDATE

#### MODELS: 1997-99 BUICK PARK AVENUE, RIVIERA 1997-99 CADILLAC SEVILLE 1997-99 OLDSMOBILE AURORA

THIS BULLETIN IS BEING ISSUED TO REVISE THE SPECIAL TOOLS AND EQUIPMENT PORTION OF SECTION 3 - FRONT SUSPENSION, IN THE SERVICE MANUAL.

A NEW BALL JOINT SEPARATOR TOOL HAS BEEN DEVELOPED IN ORDER TO FIT BETWEEN THE DRIVE AXLE AND THE LOWER BALL JOINT STUD ON THE ALUMINUM STEERING KNUCKLE ASSEMBLIES. THE NEW BALL JOINT SEPARATOR REMOVER TOOL (J 43828) DIFFERS SLIGHTLY IN APPEARANCE FROM THE ORIGINAL, THEREFORE, A NEW ILLUSTRATION IS NOT INCLUDED.

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1998 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.