Cooling System Components. Cadillac Concours 1997

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Engine Compartment Fuse/Relay Center | Left hand of the engine compartment, near the front strut tower | 8A-201-4 Fig 9 | --
Engine Cooling Fan Relay 1 | Center front of the engine compartment, on the lower radiator support, near the cooling fans | 8A-201-2 Fig 5 | 8A-202-79
Engine Cooling Fan Relay 2 | Center front of the engine compartment, on the lower radiator support, near the cooling fans | 8A-201-2 Fig 5 | 8A-202-79
Engine Cooling Fan Relay 3 | Center front of the engine compartment, on the lower radiator support, near the cooling fans | 8A-201-2 Fig 5 | 8A-202-79
LH Cooling Fan Motor | Left hand front of the engine compartment, behind the radiator | 8A-201-2 Fig 5 | 8A-202-87
Powertrain Control Module (PCM) | Left hand front corner of the engine compartment, under the air cleaner housing | -- | Engine Controls
RH Cooling Fan Motor | Right hand front of the engine compartment, behind the radiator | 8A-201-2 Fig 5 | 8A-202-87
RH Maxifuse® Block | Left hand of the engine compartment, near the engine compartment fuse/relay center | 8A-201-4 Fig 9 | --
G107 | Lower left hand front corner of the engine, below the thermostat housing | 8A-201-16 Fig 31 | --
S117 | Engine harness, approx 34 cm from the RH cooling fan connector | 8A-201-2 Fig 5 | --
S118 | Engine harness, approx 16.5 cm from the powertrain control module connector breakout | 8A-201-16 Fig 31 | --
S129 | Engine harness, approx 4 cm from the C129 connector breakout | 8A-201-2 Fig 5 | --
S130 | Engine harness, approx 6.5 cm from the EBTCM connector breakout | 8A-201-2 Fig 5 | --