DRIVER'S FLEET COLD/POOR HEAT DISTRI. (REPL. FLOOR OUTLET). Cadillac Concours 1994

For 1990-2009 cars

# DRIVER'S FLEET COLD/POOR HEAT DISTRI. (REPL. FLOOR OUTLET)

#### SUBJECT: DRIVER'S FEET COLD/POOR HEAT DISTRIBUTION (REPLACE FLOOR OUTLET ASSEMBLY)

#### MODELS: 1992-94 CADILLAC ELDORADO AND SEVILLE 1994 CADILLAC CONCOURS AND DEVILLE

#### VIN BREAKPOINTS:

FOR 1994 MODELS:

ELDORADO - 609809 SEVILLE - 822386 CONCOURS/DEVILLE - 237594

VEHICLES BUILT AFTER THESE BREAKPOINTS WERE ASSEMBLED WITH THE NEW DESIGN FLOOR OUTLET ASSEMBLY.

#### CONDITION:

SOME OWNERS MAY COMMENT THAT THERE IS POOR HEAT DISTRIBUTION TO THE FLOOR AREA OF THE DRIVER'S COMPARTMENT RESULTING IN THE DRIVER'S FEET GETTING COLD.

#### CORRECTION:

REPLACE THE FLOOR AIR OUTLET ASSEMBLY, P/N 3546494, USING THE PROCEDURES FOUND IN SECTION 1B OF THE APPROPRIATE SERVICE MANUAL. THE NEW PART CAN BE IDENTIFIED BY VANES IN THE OUTLETS. THE OLD DESIGN HAS NO OUTLET VANES.

PARTS ARE EXPECTED TO BE AVAILABLE ON JULY 11, 1994.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: D1517 LABOR TIME: 2.1 ADD: .7 (FOR "E/K" WITH FULL CONSOLE)

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.