Component and System Description. Cadillac Concours 1997

For 1990-2009 cars

The mechanical components of this unit are as follows:

• | A torque converter with a Torque Converter Clutch (TCC)

• | A drive link assembly

• | 4th and Lo/Reverse band assemblies

• | Forward, Coast, 2nd and 3rd multiple disc clutches

• | Two planetary gear sets

• | Two sprag clutches (Forward and 2nd)

• | One roller clutch (Lo)

• | Three fluid pumps

• | Two control valve assemblies

• | A final drive assembly with a bolted on case extension

The electrical components of this unit are as follows:

• | Two shift solenoid valves, 1-2 and 2-3

• | A Torque Converter Clutch Solenoid valve

• | A transmission Pressure Control Solenoid valve (PC Sol. Valve)

• | An Automatic Transmission Fluid Temperature sensor (TFT)

• | Two speed sensors: Input and Vehicle Speed Sensor

• | An Automatic Transmission Fluid Pressure Manual Valve Position switch (TFP Val Position Sw)

• | An Automatic Transmission Wiring Harness