Ignition Coil Module Removal. Cadillac Concours 1997

For 1990-2009 cars

1. Disconnect the remaining spark plug wires from the spark plugs.
2. Remove all spark plug wires from the ignition coil pack and store in a safe location.
3. Disconnect the ground strap (1) from the cylinder head.
4. Remove the ignition coils and control module retaining bolts.
5. Remove the ground strap.
6. Remove the ignition coils and control module (2) as an assembly from the camshaft cover.