Transaxle Seized. Cadillac Concours 1996

For 1990-2009 cars

#### Transmission Seized

Checks | Action
--- | ---
Cooler Circuit Lines | Blocked or leaking
Cooler Fittings | Blocked or leaking
Spacer Plate/Gaskets | Holes missing, off location

Scavenger Pipe

• | Damaged, clogged

• | Poor seal at pipe

Control Valve Bodies | Loose, broken or missing bolts
Transmission Fluid Filter | Sitting in side cover
Filter Seal | Cut damaged neck seal
Left and Right Scavenge Screens | Clogged or not seated in case