Engine Electrical Components. Cadillac Concours 1997

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Battery | Right hand front of the engine compartment, near the engine coolant reservior | 8A-201-8 Fig 16 | --
Generator | Right hand front corner of the engine, near the battery | 8A-201-11 Fig 22 | 202-82
Ignition Switch | Under the left hand of the instrument panel, on the base of the steering column | 8A-201-25 Fig 48 | --
Instrument Panel Cluster (IPC) | Left hand of the instrument panel, above the steering column | 8A-201-22 Fig 42 | --
Park/Neutral Position (PNP) Switch | Left hand of the transaxle, below the throttle body | 8A-201-16 Fig 32 | 202-97
Powertrain Control Module (PCM) | Left hand front corner of the engine compartment, under the air cleaner housing | -- | Engine Controls
RH Maxifuse® Block | Left hand of the engine compartment, near the engine compartment fuse/relay center | 8A-201-4 Fig 9 | --
Starter Enable Relay | Left hand of the engine compartment, near the right hand maxifuse® Block | 8A-201-4 Fig 9 | 202-104
Starter Motor | Center of engine under intake manifold | -- | --
Starter Solenoid | Center of engine under intake manifold, on starter motor | -- | --
C101 | Forward of the left hand strut tower, near engine compartment fuse/relay center | 8A-201-4 Fig 9 | 8A-202-0
C131 | Right hand rear corner of the engine, near the cam cover | 8A-201-19 Fig 38 | 202-15
C202 | Under left hand of the instrument panel, near the base of the steering column | 8A-201-25 Fig 47 | 202-5
G100 | Right hand front corner of the engine compartment, on the radiator support | 8A-201-8 Fig 16 | --
G105 | Right hand front corner of the engine, near the generator | 8A-201-20 Fig 39 | --
P101 | Left hand rear of the engine compartment, near the strut tower | 8A-201-5 Fig 11 | --
S121 | Engine harness, approx 32.5 cm from the starter enable relay | 8A-201-4 Fig 9 | --