Secondary Pump Disassemble. Cadillac Concours 1996

For 1990-2009 cars

1. Remove the following parts:

• | The retainer clip (215)

• | The pump ball seat (217)

• | The cut off ball (216)

2. Remove the following parts:

• | The retainer clip (215)

• | The pressure regulator boost valve sleeve (214)

• | The pressure regulator boost valve (213)

• | The pressure regulator valve spring (212)

• | The pressure regulator spring retainer (210)

• | The pressure regulator valve (211)