Accumulator Housing Disassemble. Cadillac Concours 1997

For 1990-2009 cars

1. Remove the following parts:

• | The two snap rings (349) from the top side of the accumulator housing (944)

• | The 1-2 accumulator assembly (968-970, 973)

• | The 3-4 accumulator assembly (975-977, 950)

2. Inspect the accumulator pistons for scratches or damage. Inspect the accumulator piston pins for scoring.
3. Remove the following parts:

• | The five 8-mm cover bolts (966)

• | The accumulator housing cover (965)

• | The gasket (964)

• | The forward accumulator assembly (960-963)

• | The reverse accumulator assembly (946-949)

4. Inspect the accumulator pistons (946, 960) and the accumulator piston pins (948, 962) for scoring or damage.