No First Gear. Cadillac Concours 1996

For 1990-2009 cars

Checks | Causes
--- | ---

1-2 and/or 2-3 Shift Solenoid Valve

• | Debris

• | Pinched or damaged wires

• | Inoperative

Checkball in Housing | Leaking
Detent Lever | Misaligned
Forward Clutch Piston | Cracked or damaged
Forward Clutch Piston Seals | Leaking, cut or rolled
Forward Clutch Plates | Burned, damaged
Forward Sprag | Damaged, not holding
FWD/Coast Housing | Broken or spline damage
Lo Roller Clutch | Worn or damaged
Manual Valve | Misaligned
Oil Transfer Sleeve | Misaligned, damaged, leaking