For 1990-2009 cars

# LABOR TIME GUIDE UPDATED INFORMATION

In an effort to provide the most current LTG information available to Cadillac dealers, an updated listing of LTG time/text changes will be published between microfiche revisions. Listed below are revised or new Labor Operations that have changed since the last microfiche revision.

Operation Operation Description Number Model(s) Time Year(s) ----------- ------ -------- ---- ------- Hood Refinish Complete A0357 J 1.5 86 & 87

Fender, Front (Complete) Color Coat Right A0681 J .6 86 & 87 Left A0681 J .6 86 & 87 Refinish J Right A0690 J .8 86 & 87 Left A0691 .8 86 & 87

Door, Front (Between Belt and Side Molding) Right A1190 D .9 86 & 87 Left A1191 4 Door D .9 86 & 87

Door Rear A1531 ADD: To Refinish Window Frame C .3 86 & 87 To Refinish Window Frame D .4 86 & 87 To Refinish Window Frame J .3 86 & 87

Quarter (Below Lower Molding, Rear of Wheel Opening) Color Coat Right A2120 J .3 86 & 87 Color Coat Left A2121 J .3 86 & 87 Refinish Right A2130 J .4 86 & 87 Refinish Left A2131 J .4 86 & 87

Cover, Rear Bumper Color Coat One Piece (*Material A3268 E,K *AE 86 & 87 Allowance)

Hoses, Air Distribution - R&R or RepLace

To Right Side Defroster D1544 J .3 86 & 87 To Left Side Defroster D1545 J 1.0 86 & 87

Compressor Assembly-Replace D4440

ADD: Al! To Flush Complete System Model R-11 ALL 1.8 Years

Gear Assembly, Power E9720 Steering - R&R

#### ADD:

To Recondition P/S Gear J 1.1 86 & 87 (Complete)

Relay, Pump (ABS) - Replace H2475 C .2 86 & 87

Fuel System - Clean & Flush L100 E,K 1.7 86 & 87

Bulb, Lamp - Replace Composite Headlamp Right N0440 C .2 87 Right J .2 86 & 87 Left N0441 C .2 87 Left J .2 86 & 87

Pump Assembly - Washer N3860 C,E,K .3 86 & 87 R&R or Replace

Heater, Engine Block R4600 C .8 86 & 87 Replace D .7 86 & 87 E .9 86 & 87 J .7 86 & 87 K .9 86 & 87

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.