For 1990-2009 cars

# LOOSE LACE AROUND FRONT DOOR OUTER FRAME MOLDING

#### VEHICLES AFFECTED: DE VILLES AND FLEETWOODS (C)

Some 19B7 De Villes and Fleetwoods may experience loose trim lace at the front door exterior frame moulding. This condition may be caused by excessive gap between the moulding lace and the front door (compare figures 1 and 2).

To repair this condition, use the following procedure:

1. Remove door trim panel as specified on page 5C-1 of the 1987 Body Service Manual.

2. Remove outside mirror as specified on page 5C-25 of the 1987 Body Service Manual.

3. Remove front door outer frame moulding as specified on page 5C-9 of the 1987 Body Service Manual.

4. Using a razor blade or, equivalent, remove the inside lip of the trim lace at the forward radius of the outer frame moulding as shown in figure 3.

5. Bond the lace" to the moulding with several drops of Loctite Quick Gel, SGG-A or equivalent.

6. Reinstall front door outer rdoulding as specified on page 5C-9 of the Body Service Manual.

#### Note: Properly position moulding to fit recess in door outer panel.

7. Reinstall outside mirror as specified on page 5C-25 of the 1987 Body Manual.

#### NOTE: Tighten the forward attaching nut first, then the two rearward nuts.

8. Reinstall door trim panel as specified on page 5C-1 of the Body Service Manual.

Use the most applicable labour operation from the Canadian Labour Time Guide and claim .9 hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.