For 1990-2009 cars

# METHOD OF VERIFYING ' GOOD ELECTRICAL SYSTEM GROUND '

#### VEHICLES AFFECTED: ALL MODELS

When diagnosing electronic systems for incorrect operation, it is often necessary to verify that ground circuits are good. This article is intended to clarify what is meant by the term "good ground" and the preferred tools and methods for verifying it.

A "good ground" is a ground circuit that has a resistance of zero OHMS.

Ground circuit resistance can be measured in OHMS using a digital volt OHM meter (DVOM). When using a DVOM, it must be set on the 200 OHM scale to obtain an accurate measure of the circuit resistance. Many meters have both a 200 OHM scale and a 200 K scale. The 200 K scale will not measure zero OHMS accurately. If you are not sure how the meter is to be set for the 200 OHM scale, refer to the meter operating instructions for proper settings. If the meter is an autoranging or self-scaling meter, read the meter carefully to be sure which scale it is setting itself to.

Before measuring resistance in any circuit, the resistance of the meter should be measured by touching the leads together. A meter with a good battery and leads in good condition will read less than .2 OHMS usually zero. If the leads measure anything more, an accurate measure of the circuit resistance may not be possible.

Always remember - resistance cannot be measured accurately on a "live" circuit, All current flow through a circuit must be stopped by disconnecting its power source before measuring resistance.

Ground circuit resistance can also be checked by measuring the voltage drop across the circuit with a DVOM set on, the 2 volt scale. The voltage drop will be zero across a "good ground" circuit.

Remember, fully understand a meter's functions before using it!

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.