For 1990-2009 cars

# DISPLAYS BLANK INTERMITTENLY ON COLD START UPS

SOME 1988 DEVILLES AND FLEETWOODS MAY EXPERIENCE A CONDITION OF ALL DISPLAYS BLANKING DURING COLD AMBIENT TEMPERATURES FOR ONLY A FEW MINUTES AFTER START UP. THIS CONDITION MAY BE CAUSED BY AN INTERMITTENT OPEN IN THE RETAINED ACCESSORY POWER (RAP) RELAY #2. TO REPAIR THIS CONDITION REPLACE THE RELAY.

FOR WARRANTY PURPOSES USE LABOR OPERATION N2895 AT .2 HOUR.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.

COPYRIGHT 1989 CADILLAC MOTOR CAR DIVISION, GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.