For 1990-2009 cars

# SERVICEMAN BULLETIN UPDATES CORRECTIONS/CHANGES LISTED

#### MODELS AFFECTED: 1982-1984 CIMARRONS 1984 DEVILLES AND FLEETWOOD BROUGHAMS 1982-1984 SEVILLES AND ELDORADOS 1985 FWD DEVILLES AND FLEETWOODS

The listed Serviceman Bulletins require the following corrections. Please update your bulletins to include these changes.

Serviceman Bulletin Correction --------- ---------- The heading should read:

Bulletin No. T 85-4 Bulletin No. T 85-4 File in Group 3D 3D Number 1 4 Date Sept.'84 Sept.'84 Models Affected* 85 B,D

Bulletin No. T 81-68A The part number 7840380 in the second File in Group 3B paragraph of Section "A. Power Steering Number 5 Valve Ring Wear" is incorrect and Date June'84 should read: Models Affected 82-84 G part number 7846635.

Bunetin No. T-85-38 The second paragraph should be changed File in Group 7 to read: Number 115 Starting on April 25, 1984 (Julian date Date Jan.'85 116) on AA and AP models... Models Affected 84 M,W

Bulletin No. T-85-44 The gaskets listed in this bulletin, P/N's File in Group 7 8639856 and 8639857, are now available as Number 116 a kit, P/N 8635976. Also an "E" clip Date Jan.'85 retainer, P/N 9431762, is required to Models Affected 84 L,S properly assemble the 3-4 accumulator piston (Figure 4).

Bulletin No. T-84-38A Steps # 3 through 9 of the "Service File in Group 7 Procedure" no longer apply to correcting Number 93 the delayed engagement condition. In Date Mar.'84 addition, the correct part number for the Models Affected 82-83 L,S pump intake check valve should be: 8635971 not 6839810 or 8639810.

*B-Deville (FWD), D-Fleetwood (FWD), G-Cimarron, Eldorado, M-Deville (RWD), S-Seville, W-Brougham

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.