For 1990-2009 cars

# CLEANING PROCEDURES: CAMBRIA AND SIMULATED CONVERTIBLE TOP

When cleaning Cambria and Simulated Convertible tops, the following procedures should be followed:

1. Wash material with a mild non detergent soap, (GM Multi-Purpose cleaner, part number 1050429 or equivalent) and a soft bristle brush.

#### CAUTION:

Stiff bristled brushes may damage top material.

2. Rinse with water and let dry. Avoid drying roof with materials that may leave lint.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.