For 1990-2009 cars

# INSTRUMENT PANEL PAD GLARE

#### SUBJECT: INSTRUMENT PANEL PAD GLARE (REPLACE PAD)

#### MODELS: 1993-95 CADILLAC FLEETWOOD PRIOR TO VIN BREAKPOINT SR710282

#### CONDITION:

SOME OWNERS MAY COMMENT ABOUT A VEILING GLARE (REFLECTION) FROM THE TOP SURFACE OF THE I/P PAD ONTO THE WINDSHIELD, WITH LIGHT GRAY, LIGHT NEUTRAL OR TAUPE COLOR INSTRUMENT PANEL PADS.

#### CORRECTION:

REPLACE THE PAD FOLLOWING INSTRUCTIONS IN THE SERVICE MANUAL, SECTION 8C-23.

COLOR P/N

LIGHT GRAY (14I) 10281085 LIGHT NEUTRAL (52I) 10281086 TAUPE (54I) 10281087

#### PART INFORMATION:

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE: LABOR OPERATION: C2510 USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.