For 1990-2009 cars

# SERVICE ENGINE LIGHT (CODE 22) DIAGNOSIS PROCEDURES

#### SUBJECT: SERVICE ENGINE SOON LIGHT (CODE 22) (PROCEDURE/DIAGNOSTICS REPLACE TPS)

VEHICLE APPLICATIONS: 1991-92 B/D/F CARS, C/K/R/V/P/S/T/G/M/L AND U

THIS BULLETIN CANCELS AND REPLACES PRODUCT SERVICE BULLETINS 91-650-101 and 91-6-118.

This bulletin pertains to the 5.0L and 5.7L engine for passenger cars and 4.3L/3.lL, 5.0L/5.7L and 7.4L engines for light duty trucks.

#### Condition:

--------- Some owners of the above vehicles may comment on a Service Engine Soon Light - Code 22 - Throttle Position Sensor low. Additional comments may include no upshift to 4th gear, no TCC, harsh transmission shifts, or poor idle quality. These conditions may be more prevalent after initial startup.

#### Cause:

----- The above concerns may result from an intermittent electrical contact inside the Throttle Position Sensor (TPS).

#### Correction:

---------- If any of the subject conditions are found, complete the following procedure:

1. Perform the normal diagnostics per Section 6E of the Service Manual.

2. Check TPS/ECM connectors per Product Service Bulletin 91-8-135.

3. If no problems are found using the normal 6E diagnostics or the bulletin, replace the TPS with a new TPS kit, P/N 17112679 per the procedure in Section 6E of the Service Manual. The new TPS will have a yellow dot at the connector area for easier identification.

Part is currently available from CANSPO.

#### Note: The lack of 4th gear, no TCC and harsh transmission shift concerns are only associated on truck applications with the HYDRA-MATIC 4L80-E (4 speed automatic) electronic transmission.

Use applicable labour operations and times.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.