For 1990-2009 cars

# A/C COMPRESSOR TOOL MOD. REWORK INSTALLER TOOL

#### VEHICLES AFFECTED: 1985 Models

When removing the clutch plate and hub assembly, the shaft key may interfere with the forcing screw. A new forcing screw insert J-33013-3 (Part of J-33013-B) eliminates the Possibility of key interference. See Product Service Bulletin number 84-1-112 dated oct. 15/84 for tool J-33013 modification.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.