PAINT INFORMATION - 1987 MODEL SUPPLIERS,PAINT TYPES LISTED. Cadillac Limousine 1987

For 1990-2009 cars

# PAINT INFORMATION - 1987 MODEL SUPPLIERS,PAINT TYPES LISTED

The listings of 1987 paint codes contained in this bulletin will enable dealers to order the necessary paint materials required for effective field repairs.

The list of colors indicates the suppliers' ordering codes for exterior, interior, vinyl roof moldings, and paint stripe colors.

Listed below is a current listing of the various Cadillac Assembly Plants and their suppliers. It should be noted, however, that paint suppliers are subject to change.

Assembly Plant Paint Type Paint Supplier Paint Codes -------------- ---------- -------------- -----------

Fleetwood Dispersion Lacquer Inmont All

Hamtramck B/C C/C Enamel Dupont All

Hamtramck (Allante) B/C C/C Enamel PPG All

Orion B/C C/C Enamel PPG All

Janesville Dispersion Lacquer DuPont All

Other manufacturers produce service paint which could perform satisfactorily for field repairs. Paint suppliers in your area can provide you with information regarding these materials.

The paint listed in this bulletin is (or soon will be) available from local paint suppliers.

TEXT ZONE 1987 MODEL PAINT INFORMATION EXTERIOR --------- Paint Color PPG/ Martin- Code Name WA# Dupont Ditzler Senour ---- ---- --- ------ ------- ------ 08 M.K.Pink 7795 2304 70748 99-6081 11 White 3967 5338 2058 30-3929

12 Silver Met. 8535 B8501 3746 30-5371 13S Silver Met.C/C 9021 D8590 3822 30-5491 14 Black Met.C/C 8767 B8701 3961 30-35877 15 Med.Gray Met. 8573 B8502 3749 30-5372 17 Pearl Gray 9057 B8702 3963 32-35878 19 Black 848 99S 9000/9300 3069

22 Lt. Sapphire Blue Met.C/C 8966 B8703 3964 30-35879 25 Lt. Blue Met. 8574 B8503 3754 30-5373 26 Lt. Sapphire Blue Met. 8964 B8704 3966 30-35865 28 Black Sapphire Met. C/C 8743 B8618 3885 30-5520 29 Dk. Sapphire Blue Met. 9970 B8706 3968 30-35866 30 Silver Met.C/C 9065 D8720 4010 37008 31 Dk. Blue Met. 8592 B8504 3760 30-5441 33 Lt. Driftwood Met.C/C 9022 B8707 3970 30-35905 38 Sungold C/C 8758 B8611 3887 30-5522 40 White C/C 8554 B8469 3680 30-5295 41 Black C/C 8555 99S 9700 30-5296 45 Maroon Met.C/C 9067 D8721 4012 73010 46 Gold Met.C/C 9071 D8723 4011 37009 48 Black Emerald Met.C/C 8747 B8608 3888 30-5482 49 Dk. Saxony Green Met. 8972 B8709 3975 32-35867 54 Yellow Beige 8525 B8521 3769 30-5437 55 White Met. Tri-Coat 9069 D8722 4013B/C 37011 4014T/C 57 Very Dk. Chestnut F/M 9146 B8724 3978 32-36346 58 Lt. Chestnut Met. 8575 B8507 3772 30-5387 62 Dk. Chestnut Met. 8593 B8508 3776 30-5389 63 Lt. Driftwood C/C 8744 B8603 3894 30-5481 72 Med. Garnet Red Met. C/C 8979 B8713 3986 30-35894 75 Med. Garnet Red Met. 8980 B8715 3988 32-35871 76 Dk. Garnet Red Met. C/C 8984 B8716 3989 30-35895 78 Med. Rosewood Met. 8986 B8717 3991 30-35873

Paint Color Sherwin-Williams R-M Code Name ACME/Rogers Inmont ---- ---- ----------- ------ 08 M.K.Pink 34/35-3442 12899 11 White L10A-2864 2080 5644 12 Silver Met. 34380 15001 13S Silver Met.C/C 35369 15365 14 Black Met.C/C 35877 17002 15 Med.Gray Met. 34381 15004 17 Pearl Gray 35878 17001 19 Black L10B-1738 A946 3000/4590 P403,M403 22 Lt. Sapphire Blue Met.C/C 35879 17003 25 Lt. Blue Met. 34382 15009 26 Lt. Sapphire Blue Met. 35865 17005 28 Black Sapphire Met. C/C 35313 16003 29 Dk. Sapphire Blue Met. 35866 17007 30 Silver Met.C/C 37008 * 31 Dk. Blue Met. 34875 15014 33 Lt. Driftwood Met.C/C 35905 17009 38 Sungold C/C 35314 16005 40 White C/C 33755 13570 41 Black C/C 33756 13572 45 Maroon Met.C/C 37010 * 46 Gold Met.C/C 37009 * 48 Black Emerald Met.C/C 35315 16006 49 Dk. Saxony Green Met. 35867 17012 54 Yellow Beige 34861 15023 55 White Met. Tri-Coat 37011 * 57 Very Dk. Chestnut F/M 36346 17031 58 Lt. Chestnut Met. 34396 15026 62 Dk. Chestnut Met. 34398 15030 63 Lt. Driftwood C/C 35310 16011 72 Med. Garnet Red Met. C/C 35894 17021 75 Med. Garnet Red Met. 35871 17022 76 Dk. Garnet Red Met. C/C 35895 17023 78 Med. Rosewood Met. 35873 17024

1987 MODEL PAINT INFORMATION INTERIOR Cont. -------------- Paint Color PPG/Ditzler PPG/Ditzler PPG/Ditzler Code Name WA# Dupont Low Gloss Semi-Gloss UCV ---- ---- --- ------ ---------- ---------- --- 50AN Light Yellow 7042 C8388-5 DEG - 82674 2-580 C8365-12 DEG 50CN Very Dk Yellow 8804 C8664-305-5 DEG - 82631 2-1168 C8664-306-12 DEG 60AN Lt. Driftwood 8782 C8623-5 DEG 25800 25644 2-1169 C8615-12 DEG 60CN Dk. Driftwood 8790 C8673-305-5 DEG - 25648 2-1170 C8673-306-12 DEG 62AN Light Saddle 7769 C8590-5 DEG 25580 25230 2-1025 C8352-12 DEG 62CN Dark Saddle 8613 C8569-5 DEG 25570 25503 2-1126 C8551-12 DEG 72CN Carmine 8577 C8563-5 DEG 72947 72776 2-1282 C8540-12 DEG - 75CN Dk. Rosewood 8843 72847 2-1216 C8774-12 DEG - 78CN Garnet Red 8781 C8624-5 DEG 72799 2-1173 C8616-12 DEG 79CN Dk. Claret 4887 C8560-5 DEG 51085 51170 2-479 C8537-12 DEG 82CN Med. Dark Gray 8247 C8556-5 DEG 33873 33665 2-1048 C8447-12 DEG 82DN Dark Gray 8595 C8597-5 DEG 33874 33824 2-1125

83BN Med. Amethyst 8831 C8550-12 DEG - 16149 2-1240 C8772-12 DEG 83CN Dk. Amethyst 8838 C8791-305-5 DEG 16322 16150 2-1231

Paint Color Martin- Sherwin-Williams R-M Code Name Senour ACME/Rogers Inmont ---- ---- ------ ------------ ------- 50AN Light Yellow 32-16992-5 DEG 32351-5 DEG 11528-5 DEG 32-17030-12 DEG 33778-12 DEG 9558-12 DEG 50CN Very Dk Yellow 32-17141-5 DEG 35440-5 DEG 16050-5 DG 32-17152-12 DEG 35473-12 DEG * 60AN Lt. Driftwood 32-17135-5 DEG 35434-5 DEG 17093-5 DEG 32-17129-12 DEG 35428-12 DEG 16056-12 DEG 60CN Dk. Driftwood 32-17138-5 DEG 35437-5 DEG 16048-5 DEG 32-17150-12 DEG 35471-12 DEG 17087-12 DEG 62AN Light Saddle 32-17086-5 DEG 34729-5 DEG 16043-5 DEG 32-16912-12 DEG 32996-12 DEG 13180-12 DEG 62CN Dark Saddle 32-17081-5 DEG 34612-5 DEG 15096-5 DEG 32-17072-12 DEG 34603-12 DEG 16053-12 DEG 72CN Carmine 32-17076-5 DEG 34607-5 DEG 16046-5 DEG 32-17085-12 DEG 34639-12 DEG 15084-12 DEG 75CN Dk. Rosewood 32-36572-5 DEG 36572-5 DEG 17098-5 DEG 32-36474-12 DEG 36474-12 DEG 17097-12 DEG 78CN Garnet Red 32-17134-5 DEG 35433-5 DEG 17085-5 DEG 32-17147-12 DEG 35468-12 DEG 16055-12 DEG 79CN Dk. Claret 32-16751-5 DEG 30814-5 DEG 12818-5 DEG 32-17084-12 DEG 34638-12 DEG 8763-12 DEG 82CN Med. Dark Gray 32-16965-5 DEG 33769-5 DEG 14088-5 DEG 32-16949-12 DEG 33714-12 DEG 14009-12 DEG 82DN Dark Gray 32-17080-5 DEG 34611-5 DEG 15095-5 DEG 32-17071-12 DEG 34602-12 DEG 15268-12 DEG 83BN Med. Amethyst 32-36570-5 DEG 36570-12 DEG 17109-5 DEG 32-36471-12 DEG 36471-12 DEG 17090-12 DEG 83CN Dk. Amethyst 32-36501-5 DEG 36501-5 DEG 17091-5 DEG

#### NOTE: Painted parts on the instrument Panel have a 5 DEG gloss finish and the steering column parts have a 12 DEG gloss finish.

* Not Available

1987 MODEL PAINT INFORMATION EXTERIOR cont. -------------- Paint Color PPG/ Martin- Code Name WA# Dupont Ditzler Senour ---- ---- --- ------ ------- ------ 79 Dk. Red Met. 8529 B8509 3786 30-5396 80 Lt. Rosewood Met. C/C 8992 B8718 3993 30-35898 82 Med. Rosewood Met. C/C 8990 B8719 3994 30-35896 83 Med Sapphire Blue F/M/C/C 8993 B8720 3995 30-35900 84 Gun Metal Met. C/C 7782 B8403 3667 30-5313 85 Med. Blue F/M 8541 B8520 3789 30-5399 88 Dk.Gray Met. 8600 B8517 3788 30-5398 89 Autumn Maple F/M 8237 B8385 3532 30-5244 91 Lt. Amethyst F/M C/C 8995 B8722 3997 30-35902 96 Dk. Driftwood F/M C/C 8765 B8605 3906 30-5486 98 Chamois F/M C/C 8565 B8616 3908 30-5404 99 Dk. Amethyst Met. C/C 8996 B8723 3998 30-35904

Paint Color Sherwin-Williams R-M Code Name ACME/Rogers Inmont ---- ---- ----------- ------ 79 Dk. Red Met. 34405 15040 80 Lt. Rosewood Met. C/C 35898 17027 82 Med. Rosewood Met. C/C 35896 17026 83 Med Sapphire Blue F/M/C/C 35900 17028 84 Gun Metal Met. C/C 33936 14066 85 Med. Blue F/M 34408 15043 88 Dk.Gray Met. 34407 15042 89 Autumn Maple F/M 33074 13131 91 Lt. Amethyst F/M C/C 35902 17029 96 Dk. Driftwood F/M C/C 35324 16024 98 Chamois F/M C/C 34413 16026 99 Dk. Amethyst Met. C/C 35904 17030

#### NOTE: C/C = Basecoat/Clearcoat F/M = Firemist * = Not Available 1987 MODEL PAINT INFORMATION INTERIOR -------- Paint Color PPG/Ditzler PPG/DitzLer PPG/Ditzler Code Name WA# Dupont Low Gloss Semi-Gloss UCV ---- ---- --- ------ --------- ---------- --- 11N White 3835 C8622-5 DEG -- 90232 -183 C8536-12 DEG 13AN Lt. Pearl Gray 8848 C8768-12 DEG -- 34087 2-1230

19N Black 848 4428-5 DEG 9433 9640 -120 C8535-12 DEG

20DN Very Dk Sapphire 8841 C8770-12 DEG -- 16202 2-1215

27CN Dark Blue 8576 C8562-5 DEG 16092 15886 2-1098 C8539-12 DEG 48BN Med. Emerald 8796 C8621-5 DEG -- 45898 2-1165 C8614-12 DEG 48DN Dark EmeraLd 8788 C8661-305-5 DEG -- 45890 2-1166 C8661-306-12 DEG

Paint Color Martin- Sherwin-Williams R-M Code Name Senour ACME/Rogers Inmont ---- ---- ------ ----------- ------ 11N White 32-17172-5 DEG 32-35574-5 DEG 11526-5 DEG 32-17029-12 DEG 32-33777-12 DEG 4402-12 DEG 13AN Lt. Pearl Gray 32-36573-5 DEG 36573-5 DEG 17084-5 DEG 32-36472-12 DEG 36472-12 DEG 17101-12 DEG 19N Black 32-16615-5 DEG J4-8677-5 DEG 12812-5 DEG 32-16918-12 DEG 92387-5 DEG 4401-12DEG 33024-12 DEG 20DN Very Dk Sapphire 32-36571-5 DEG 36571-5 DEG 17095-5 DEG 32-36479-12 DEG 36479-12 DEG 17094-12 DEG 27CN Dark Blue 32-17075-5 DEG 34606-5 DEG 16045-5 DEG 32-17067-12 DEG 34598-12 DEG 15080-12 DEG 48BN Med. Emerald 32-17140-5 DEG 35439-5 DEG 17082-5 DEG 32-17131-12 DEG 35430-12 DEG 16059-12 DEG 48DN Dark Emerald 32-17137-5 DEG 35436-5 DEG 16047-5 DEG 32-17149-12 DEG 35470-12 DEG 17086-12 DEG

#### 1987 CADILLAC PAINT STRIPE COLORS

GM Paint Color Fisher R-M PPG/ Code Name "WA" No. Inmont DuPont Ditzler ---- ---- -------- ------ ------ ------- 09A Lt. Quartz 8810 16075 C-8644 72803 11A White 3967 2080 5338 2058

14A Lt. Gray 8670 15165 C-8529 3856 18A Gun Metal 8291 14036 C8441 33750 19A Black 848 A946 99 9000/9300

20A Lt. Sapphire 9193 17057 C8786 16319 21A Dk. Sapphire 9103 17055 C8787 16313 28A Dk. Blue 8659 15074 C8521 15892 37A Lt. Emerald 8809 16077 C8646 16081 51A Sun Gold 8758 16080 B8611 25803 55A Gold 8589 15076 D8276 25509 56A Lt.Driftwood 8744 16081 B8603 25802 57A Dk.Driftwood 8808 16082 C8640 25774 58A Lt. Chestnut 8851 16083 C8641 25775 62A Lt. Saddle 8660 15173 C8522 25551 65A Med.Chestnut 8672 15176 C8531 25552 66A Orange 8002 9500 45261 60909

67A Dk. Brown 8001 9502 45260 25088

68A Lt. Rosewood 8874 17051 C8782 51283 72A Dk. Rosewood 8872 17050 C8783 51282 73A Dk. Garnet 9106 17056 C8790 51286 75A Red 4721 4518 43592 72128

76A Garnet Red 8852 16086 C8643 51211 79A Dk. Claret 8663 15071 C8525 51167 82A Lt. Amethyst 8875 17052 C8784 51284 86A Dk. Amethyst 9081 17054 C8785 51285

GM Paint Color Martin- Sherwin-Williams Code Name Senour ACME/Rogers ---- ---- ------ ----------- 09A Lt. Quartz 32-26777 35563 11A White 32-3929 L10A-2864 5644 14A Lt. Gray 32-26729 34869 18A Gun Metal 32-26700 34102 19A Black 3069 L10B-1738 3000/4590 20A Lt. Sapphire 32-36466 36466 21A Dk. Sapphire 32-36464 36464 28A Dk. Blue 32-26722 34864 37A Lt. Emerald 32-26776 35562 51A Sun Gold 30-5522 35314 55A Gold 32-26703 34105 56A Lt.Driftwood 30-5481 35310 57A Dk.Driftwood 32-26775 35561 58A Lt. Chestnut 32-26779 35565 62A Lt. Saddle 32-26725 34865 65A Med.Chestnut 32-26731 34871 66A Orange 32-26337 J4-8728 25455 67A Dk. Brown 32-26336 J4-8727 25460 68A Lt. Rosewood 32-36460 36460 72A Dk. Rosewood 32-36459 36459 73A Dk. Garnet 32-36465 36465 75A Red 32-26272 J4-7191 11892 76A Garnet Red 32-26780 35566 79A Dk. Claret 32-26728 34868 82A Lt. Amethyst 32-36461 36461 86A Dk. Amethyst 32-36463 36463

#### 1987 CADILLAC DE VILLE AND FLEETWOOD BUMPER RUB STRIP COLOR

Paint Color PPG/ Martin- Sherwin-Williams Code Name WA# Dupont Ditzler Senour ACME/Rogers ---- ---- --- ------ ------- ----- ----------- - Med.Gray Met. 9145-50 DEG C8672 34173 32-26855 36383

Paint Color R-M Code Name Inmont ---- ---- ------ - Med.Gray Met. 16088

#### 1987 CADILLAC VINYL ROOF MOLDING COLORS

GM Paint Color Fisher R-M PPG/ Code Name "WA" No. Inmont DuPont Ditzler ---- ---- -------- ------ ------ ------- 11T White (Tuxedo) 3967 4415 5338 2-130

11T White (Elk) 8936 16110 * 2-130 13T Silver Met. 7781 14039 B8402 2-1052 18T Black Met. 8767 17065 B8701 2-1269 19T Black 848 4416 99 -120

22T Lt. Sapphire Blue Met. 8966 17066 B8703 2-1271 26T Lt. Sapphire Blue Met. 8964 17005 B8704 * 28T Black Sapphire Met. 8743 17068 B8628 2-1273 29T Dk. Sapphire Blue Met. 8970 17007 B8706 * 33T Lt. Driftwood Met. 9022 17069 B8707 2-1262 34T Lt. Blue Met. 8533 15061 B8538 2-1107 38T Sungold 8758 16104 B8611 2-1185 48T Black Emerald Met. 8747 16101 B8608 2-1186 54T Yellow Beige 8525 15184 B8521 2-1104 57T Vy. Dk. Chestnut Met. 9146 17031 B8724 2-1263 58T Lt. Chestnut Met. 8575 16097 B8507 2-1199 62T Dk. Chestnut Met. 8593 17071 B8508 2-1264 63T Lt. Driftwood 8744 16098 B8603 2-1188 72T Med. Garnet Red Met. 8979 17072 B8713 2-1268 75T Med. Garnet Red Met. 8980 17022 B8715 * 76T Dk. Garnet Red 8984 17073 B8716 2-1272 79T Dk. Red Met. 8529 15187 B8509 2-1105 82T Med. Rosewood Met. 8990 17075 B8719 2-1266 83T Med. Sapphire Blue Met. 8993 17074 B8720 2-1274 84T Gun Metal Met. 7782 14040 B8403 2-1053 85T Lt. Rosewood Met. 8992 17077 B8718 2-1285 91T Lt. Amethyst Met. 8995 17076 B8722 2-1270 96T Dk. Driftwood Met. 8765 16108 B8605 2-1196 98T Chamois Met. 8565 16096 B8616 2-1198 99T Dk. Amethyst Met. 8996 17078 B8723 2-1267

GM Paint Color Martin- Sherwin-Williams Code Name Senour ACME/Rogers ---- ---- ------ ----------- 11T White (Tuxedo) 32-26185 J4-5676/ 11510 11T White (Elk) 32-26851 35781 13T Silver Met. 32-26704 34123 18T Black Met. 32-36594 36594 19T Black 32-16082 J4-1990/ 9739 22T Lt. Sapphire Blue Met. 32-36595 36595 26T Lt. Sapphire Blue Met. 32-37031 37031 28T Black Sapphire Met. 32-36593 36593 29T Dk. Sapphire Blue Met. 32-37032 37032 33T Lt. Driftwood Met. 32-36603 36603 34T Lt. Blue Met. 32-26754 35027 38T Sungold 32-26844 35774 48T Black Emerald Met. 32-26841 35771 54T Yellow Beige 32-26763 35109 57T Vy. Dk. Chestnut Met. 32-36605 36605 58T Lt. Chestnut Met. 32-26836 35766 62T Dk. Chestnut Met. 32-26837 35767 63T Lt. Driftwood 32-26838 35768 72T Med. Garnet Red Met. 32-36596 36596 75T Med. Garnet Red Met. 32-37033 37033 76T Dk. Garnet Red 32-36597 36597 79T Dk. Red Met. 32-26760 35086 82T Med. Rosewood Met. 32-36598 36598 83T Med. Sapphire Blue Met. 32-36600 36600 84T Gun Metal Met. 32-26705 34124 85T Lt. Rosewood Met. 32-36599 36599 91T Lt. Amethyst Met. 32-36601 36601 96T Dk. Driftwood Met. 32-26848 35778 98T Chamois Met. 32-26833 35763 99T Dk. Amethyst Met. 32-36602 36602

* Not Available

#### EXTERIOR PLASTIC PARTS

All 1987 Cadillace have exterior parts made of various types of plastic materials that require specific procedures to obtain high quality refinishing results. Included in this bulletin is a chart listing the different types of plastic materials used on 1987 models. For best results when painting is required, determine the type of plastic material from the chart. Then follo w the correct paint procedure, depending upon what painting material and equipment is available.

PLASTIC TYPE SYMBOL

Thermoset Urethane RRIM Thermoplastic Urethane TPU Thermosetting Polyester UP (SMC) Thermoplastic Urethane RIM Thermoplastic Elastomer TPE Zenoy --

A. GENERAL PAINT PROCEDURE FOR EXTERIOR FLEXIBLE PLASTICS

Poiyvinylchloride (PVC), Polyurethane (PUR, TPUR, RRIM, RIM), Thermoplastic Elastomer (TPE), Thermoplastic Polyester (SMC), EPDM Rubber (Supplied in Prime).

There are a multitude of finishing systems available on the market for painting and/or repairing flexible plastic parts. Following is a general outline of painting procedures, including a list of available products. Refer to the manufacturer's literature available through your jobber for details on proper mixing and application.

1. Thoroughly clean part by washing with a suitable cleaning solvent* to remove all surface contaminates.

#### NOTICE: Previously painted parts that show signs of cracking, peeling or improper adhesion must be stripped before repainting. The old finish may be removed with any commercially available chlorinated solvent stripper or lacquer thinner.

#### NOTICE: Do not soak parts longer than necessary to remove the old paint to avoid swelling.

2. Scuff sand to an even dull appearance the entire surface to be painted with fine (400 grit or less) sandpaper and feather edge any damaged areas and rewash as in Step A.

#### NOTICE: Unpainted parts do not require sanding prior to painting, but should be thoroughly cleaned as in Step A.

3. Apply two (2) thin coats of primer when required per top coat manufacturer's recommendation and allow to compleyely dry before proceeding. (For most products, approximately 30 minutes).

4. Prepare color coat according to the manufacturer's recommendation and apply sufficient double coats to develop the proper shade. For best results, allow a few minutes flash time between each double coat and allow to completely dry before using.

5. Following is a list of some of the products available for painting flexible plastic.

PPG/Ditzler Elastomeric Primer - DPX844 PPG/Ditzler Flexative - DX369 (Permanent Flexible Urethane Additive) PPG/Ditzler Flex Additive - DX1798 (Non-Urethane Additive) DuPont (Flexlar-350S (Flexible Additive) Sherwin-Williams Multi-Flex - V6V299 Acme/Rogers Multi-Flex - 68/4068 Martin-Senour Flex Additive - 3084

* Cleaning Solvents

a. DuPont Prep-Sol b. Rinshed-MasonPre-Kleano 900 c. PPG/Ditzler Acryli-Clean DX330 d. Sherwin-Williams R7KI56 e. Acme 88;Rogers 088 f. Martin-Senour 6383

B. NYLON - Will be supplied in prime. Use the same procedure to refinish as on sheet metal parts.

C. ACRYLONNITRILE-BUTADIENE-STYRENE (ABS) - No prime required; paint with acrylic lacquer.

D. POLYESTER PARTS (UP, PBTP) - Will be supplied in prime and/or black paint. Use the same procedure to refinish or repair as on sheet metal parts .

E. POLYPROPYLENE-Interior parts.

1. Wash surface thoroughly with enamel reducer. (Do not use wax and grease removers.)

2. Apply primer immediately and allow to dry completely before color coating.

3. Color coat with lacquer or enamel reduced and applied according to the manufacturer's recommendation.

4. Materials:

Cleaning Solvent - DuPont 3812S Enamel Reducer PPG/Ditzler DTE-101 or DTE-102 "Bobcat" Enamel Reducer Primer - DuPont 3293 GM 1052364 PPG/ditzler DPX-800 Sherwin-Williams P3C24 * ACME/Rogers 524/4524* Martin-Senour 6242* * Good on polyethylene and polypropylene Parts

F. Zenoy - will be supplied in colors. Use the same procedure to refinish or repair as on sheet metal parts.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.