For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment lid lock assembly latch.
2. Remove the rear compartment lid applique, Oldsmobile only. Refer to Rear Compartment Lid Applique Replacement .
3. Remove the rivets.
4. For Oldsmobile models, remove the rear compartment lid lock cylinder and the shim.

### Installation Procedure

1. For Oldsmobile models, install the rear compartment lid lock cylinder and the shim.
2. Install the rivets.
3. Install the rear compartment lid applique, Oldsmobile only. Refer to Rear Compartment Lid Applique Replacement .
4. Install the rear compartment lid lock assembly latch. Ensure that the latch is fully seated. This action will engage the locking tabs.