For 1990-2009 cars

Component | Location | Locator View | Connector End View
--- | --- | --- | ---
AC Refrigerant Pressure Sensor | In the front of the engine compartment | HVAC Component Views in HVAC Systems with AC-Manual | HVAC Connector End Views in HVAC Systems with AC-Manual
Air Temperature Actuator | On the top right side of the IP | HVAC Component Views in HVAC Systems with AC-Manual | HVAC Connector End Views in HVAC Systems with AC-Manual
Camshaft Position (CMP) Sensor | On the top front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Crankshaft Position (CKP) Sensor | In the lower front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Cruise Control Brake Switch | Below the left side of the IP, near the steering column | Cruise Control Component Views in Cruise Control | Cruise Control Connector End Views in Cruise Control
Cruise Control Module | In the right side of the engine compartment | Cruise Control Component Views in Cruise Control | Cruise Control Connector End Views in Cruise Control
Data Link Connector | On the left side of the IP | Data Link Communications Component Views in Data Link Communications | Data Link Communications Connector End Views in Data Link Communications
Engine Coolant Level Switch | In the right side of the engine compartment | Engine Controls Component Views | Engine Controls Connector End Views
Engine Coolant Temperature (ECT) Sensor | On the top rear of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Engine Oil Pressure Sensor | On the top left of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Evaporative Emission Canister | On the top rear of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Evaporative Emission Canister Purge Valve | On the lower front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Evaporative Emission Canister Vent Solenoid | Under the rear of the vehicle | Engine Controls Component Views | Engine Controls Connector End Views
Exhaust Gas Recirculation (EGR) Valve | On the top front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Fuel Injectors | On the top front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Fuel Pump Relay | In the underhood junction block | Engine Controls Component Views | --
Fuel Tank Module | Under the rear of the vehicle | Engine Controls Component Views | Engine Controls Connector End Views
Fuel Tank Pressure Sensor | Under the rear of the vehicle | Engine Controls Component Views | Engine Controls Connector End Views
Fusible Link | On the lower front of the engine | -- | --
Generator | On the lower front of the engine | -- | --
Idle Air Control (IAC) Valve | On the top front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Ignition Coils | On the rear of engine | Engine Controls Component Views | Engine Controls Connector End Views
Ignition Control Module | On the top left of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Instrument Cluster | On the left side of the IP | Instrument Panel, Gages, and Console Component Views in Instrument Panel Gauges and Console | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel Gauges and Console
Intake Air Temperature (IAT) Sensor | On the top left side of the engine compartment | Engine Controls Component Views | Engine Controls Connector End Views
Knock Sensor | On the top left side of the engine | Engine Controls Component Views | Engine Controls Connector End Views
LH IP Junction Block | On the left side of the IP | Power and Grounding Component Views in Wiring Systems | --
Manifold Absolute Pressure (MAP) Sensor | On the top front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Mass Air Flow (MAF) Sensor | On the top left side of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Oil Life/Tire Pressure Monitor Reset Switch | In the left IP junction block | Power and Grounding Component Views in Wiring Systems | --
Post Converter Heated Oxygen Sensor (HO2S 2) | In the right side of the IP | Engine Controls Component Views | Engine Controls Connector End Views
Powertrain Control Module | Below the left side of the IP near the steering column | Engine Controls Component Views | Engine Controls Connector End Views
Pre Converter Oxygen Sensor (O2S 1) | On the top left of the engine | Engine Controls Component Views | Engine Controls Connector End Views
RH Cooling Fan Motor | In the front of the engine compartment | Engine Controls Component Views | Engine Controls Connector End Views
RH IP Junction Block | In the right side of the passenger compartment | Power and Grounding Component Views in Wiring Systems | --
Starter Motor | On the lower front of the engine | Engine Controls Component Views | --
Starter Solenoid | On the lower front of the engine | Engine Controls Component Views | --
Throttle Position (TP) Sensor | On the top front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Park/Neutral Position Switch | On the left side of the engine | Automatic Transmission Electronic Component Views | --
Underhood Junction Block | In the left side of the engine compartment | Power and Grounding Component Views in Wiring Systems | --
Vehicle Speed Sensor (VSS) | At the rear of the engine/transaxle | Engine Controls Component Views | Engine Controls Connector End Views
C101 (10 cavity) | On the left side of the engine compartment | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C102 (20 cavity) | On the left side of the engine | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200 (18 cavity) | Below the left side of the IP, near the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C300 (10 cavity) | Below the left side of the IP, near the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C413 (16 cavity) | Under the rear of the vehicle | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G102 | On the front of the engine | Harness Routing Views in Wiring Systems | --
G102 | On the lower front of the engine | Harness Routing Views in Wiring Systems | --
G103 | On the lower front of the engine | Harness Routing Views in Wiring Systems | --
G201 | On the left side of the IP | Harness Routing Views in Wiring Systems | --
G301 | On the left side of the passenger compartment | Harness Routing Views in Wiring Systems | --
P100 | In the rear of the engine compartment | Harness Routing Views in Wiring Systems | --
P200 | In the rear of the engine compartment | Harness Routing Views in Wiring Systems | --
S101 | In the injector harness, approximately 16 cm (6.3 in) from C130, towards the injectors | Harness Routing Views in Wiring Systems | --
S102 | In the engine harness, approximately 15 cm (5.9 in) from P100, towards the PCM | -- | --
S103 | In the engine harness, approximately 15 cm (5.9 in) from P100, towards the PCM | -- | --
S104 | In the engine harness, approximately 15 cm (5.9 in) from P100, towards the PCM | -- | --
S105 | In the engine harness, approximately 15 cm (5.9 in) from P100, towards the PCM | -- | --