For 1990-2009 cars

## Rear License Plate Lamp Replacement Pontiac

### Removal Procedure

1. Remove the license plate.
2. Remove the screws from the license lamp.
3. Remove the license lamp to the rear bumper fascia.
4. Remove the bulb socket from the license lamp.
5. Remove the bulb from the socket, if required.

### Installation Procedure

1. Install the bulb to the socket, if required.
2. Install the socket to the license lamp.
3. Install the license lamp to the rear bumper fascia.
4. Install the screws to the license lamp.

Tighten
Tighten the license lamp screw to 2 N·m (17 lb in).

5. Install the license plate.

## Rear License Plate Lamp Replacement Oldsmobile

### Removal Procedure

1. Remove the license plate.
2. Remove the screws from the license lamp.
3. Remove the license lamp from the rear bumper fascia.
4. Remove the bulb socket from the license lamp.
5. Remove the bulb from the socket, if required.

### Installation Procedure

1. Install the bulb to the socket, if required.
2. Install the socket to the license lamp.
3. Install the license lamp to the rear bumper fascia.
4. Install the screws to the license lamp.

Tighten
Tighten the license lamp screw to 2 N·m (17 lb in).

5. Install the license plate.