For 1990-2009 cars

#### Body Control Module (BCM)

Scan Tool Output Control | Additional Menu Selection | Description
--- | --- | ---
ALC Headlamps | Light Test | The BCM actuates the headlamps when you select ON. The headlamps should illuminate for 5 seconds
ALC Parking Lamps | Light Test | The BCM actuates the ALC park lamp relay for 5 seconds when you select ON. The park lamps should illuminate for 5 seconds.
Daytime Running Lamps | Light Test | The BCM actuates the DRL relay for 5 seconds when you select ON. The Daytime Running Lamps should illuminate for 5 seconds.
Front Fog Lamps | Light Test | The BCM actuates the FOG LAMP relay for 5 seconds when you select ON. The front fog lamps should illuminate for 5 seconds.
Interior Lamps | Light Test | The BCM actuates the interior lamp control for 5 seconds when you select ON. The foot well, and courtesy lamps should illuminate for 5 seconds.