For 1990-2009 cars

### General Description

The vehicle body are of unitized construction. The inner fender panels and the radiator support are also an integral part of the body.

### Lubrication

Lubricate the following components using Lubriplate, GM P/N 1052196 or the equivalent:

• | The primary hood latch

• | The secondary hood latch

• | The hood hinges

### Anti-Corrosion Protection

Anti-corrosion materials have been applied to the surfaces of the metal panels in order to provide rust resistance. When servicing these panels, properly re-coat the areas on this material that have been disturbed using a service-type anti-corrosion material. Refer to Paint and Coatings.