For 1990-2009 cars

Table 1: | Turn Signal/Multifunction Switch, C3
Table 2: | Washer Fluid Level Sensor
Table 3: | Windshield Washer Fluid Pump
Table 4: | Windshield Wiper Motor Assembly

#### Turn Signal/Multifunction Switch, C3

Connector Part Information |

• | 12041429

• | 5-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 92 | Windshield Wiper Motor High Speed
B | RED | 228 | Windshield Washer Pump Control
C | YEL | 143 | Accessory Voltage
D | GRY | 112 | Windshield Wiper Switch Signal 1
E | DK GRN | 113 | Windshield Wiper Switch Signal 2

#### Washer Fluid Level Sensor

Connector Part Information |

• | 12162195

• | 2-Way F Metri-Pack 150.2 Series Sealed Pull-to-Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 99 | Windshield Washer Fluid Level Signal
B | BLK | 1350 | Ground

#### Windshield Washer Fluid Pump

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 228 | Windshield Washer Pump Control
B | BLK | 1350 | Ground

#### Windshield Wiper Motor Assembly

Connector Part Information |

• | 12129126

• | 5-Way F Metri-Pack Mixed Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 150 | Ground
B | YEL | 143 | Accessory Voltage
C | PPL | 92 | Windshield Wiper Motor High Speed
D | DK GRN | 113 | Windshield Wiper Switch Signal 2
E | GRY | 112 | Windshield Wiper Switch Signal 1