For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Control Arm to Frame Bolts (Front Bushings) | 60 N·m plus 180 degrees rotation | 45 lb ft
Control Arm to Frame Bolts (Rear Vertical Bushings) | 245 N·m | 180 lb ft
Engine Frame to Body Fasteners | 191 N·m | 141 lb ft
Rear Suspension Support | 120 N·m | 89 lb ft
Suspension Crossmember to Front Bolts | 245 N·m | 180 lb ft
Suspension Crossmember to Body Rear Bolts | 70 N·m | 52 lb ft