For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Symptoms - Wiper/Washer Systems
1 | Did you review the Wiper/Washer System Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Wiper/Washer Systems
2 |

1. Turn the ignition ON.
2. Turn the windshield wiper/washer switch OFF.

Do the windshield wipers remain in the park position?

Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems

Go to Step 3

3 | Disconnect the windshield wiper/washer switch connector. Do the windshield wipers stop? | Go to Step 4 | Go to Step 5
4 | Replace the windshield wiper/washer switch. Is the repair complete? | Go to Step 6 | --
5 | Replace the windshield wiper motor module. Refer to Wiper Motor Cover Replacement . Is the repair complete? | Go to Step 6 | --
6 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3