For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement .
2. Disconnect the electrical connector from the trip odometer and reset switch.
3. Release the retainers on the trip odometer and reset switch by using a small flat-bladed tool.
4. Remove the trip odometer and reset switch from the instrument panel cluster trim plate.

### Installation Procedure

1. Align the trip odometer and reset switch to the instrument panel cluster trim plate.
2. Install the trip odometer and reset switch into retainers, by pressing into place until fully seated.
3. Connect the electrical connector to the trip odometer and reset switch.
4. Install the instrument panel cluster trim plate. Refer to Instrument Cluster Trim Panel Replacement .