For 1990-2009 cars

Thermoset Plastic Type | Type of Repair | Recommended Repair Material | Availability
--- | --- | --- | ---
Most flexible and semi fexible plastic* | Most repairs* | Compoxy Repair Material or equivalent | Dealer/Retailer
CMR-8 Composite Material Repair P/N 82091 or equivalent | Refer to local paint supplier | -- | --
* TPO, TEO, Polyolefin Plastics require the application of polyolefin adhesive primer before the repair compound is applied.