For 1990-2009 cars

### Diagnostic Aids

You cannot properly service a clutch until you know what is wrong with it. In many instances when you can not select gears can be a result of a faulty internal parts of the transmission or a faulty clutch master cylinder.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. This step explains there parts and the operation of the clutch system.

2. This step checks for problems in the transmission.

3. This step inspects for a faulty concentric slave cylinder.

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: Clutch pedal effort and clutch pedal travel are normal.
1 | Did you review the clutch symptom operations and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Clutch
2 | Go to Symptoms - Clutch . Is the clutch system OK? | Go to Step 3 | Go to Step 4
3 | Diagnose the transmission. Refer to Transmission Replacement . Does the clutch system operate properly? | System OK | Go to Step 4
4 | Check the master cylinder. Is the master cylinder worn or faulty? | Go to Step 5 | Go to Step 6
5 | Replace the clutch master cylinder. Refer to Clutch Master Cylinder Replacement Does the clutch work now? | System OK | Go to Step 6
6 | Inspect the clutch actuator. Is the clutch actuator worn or faulty? | Go to Step 7 | --
7 |

1. Replace the clutch actuator. Refer to Clutch Actuator Cylinder Replacement .
2. Operate the system in order to verify the repair.

Did you correct the condition?

System OK

Go to Diagnostic Aids