For 1990-2009 cars

### Unlock Doors

Momentarily press the UNLOCK button to unlock the driver's door only. To unlock the remaining doors, press the UNLOCK button a second time within 5 seconds. The interior lamps will illuminate for approximately 10 seconds or until the ignition is turned to the ON position. The parking lamps will flash twice to indicate unlocking has occurred.

### Lock All Doors

Press the LOCK button to lock all the doors. The interior lamps will turn off after all of the doors are closed. If all of the doors are closed, the parking lamps will flash twice and the horn will sound to indicate locking has occurred.

### Rear Compartment Lid Release

If the vehicle transaxle is in Park, a single press of the lower right transmitter Rear Compartment Release button will cause the rear compartment lid to open. The interior lamps will illuminate for approximately 10 seconds or until the ignition is turned to the ON position.

### Alarm

A single press of the lower left transmitter ALARM button will cause the interior lamps to illuminate, the horn to sound intermittently and the headlamps to flash for up to 1 minute or until one of the following occurs:

• | The Alarm button is pressed again.

• | The ignition is turned to the ON position.