For 1990-2009 cars

### Removal Procedure

1. Open the instrument panel compartment door.
2. Use a small flat-bladed tool in order to depress retainers on instrument panel compartment lamp switch.
3. Remove the instrument panel compartment lamp switch from the instrument panel compartment.
4. Disconnect the electrical connector from the instrument panel compartment lamp switch.
5. Remove the bulb from the instrument panel compartment lamp switch socket.

### Installation Procedure

1. Install the bulb into the instrument panel compartment lamp switch socket.
2. Connect the electrical connector to the instrument panel compartment lamp switch.
3. Install the instrument panel compartment lamp switch .

Press in the until retainers are fully seated.