For 1990-2009 cars

#### Engine Coolant Fan Motor (RH)

Connector Part Information |

• | 12066681

• | 2-Way F Metri-Pack 630 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 450 | Ground
B | GRY | 532 | Coolant Fan Motor Feed-Secondary

#### Engine Coolant Fan Motor (LH)

Connector Part Information |

• | 12103172

• | 2-Way F Metri-Pack 630 Series Pull to Seat (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 504 | Coolant Fan Motor Output
B | LT BLU | 409 | Coolant Fan Motor Feed

#### Engine Coolant Level Sensor

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL/BLK | 68 | Low Coolant Level Indicator Lamp Output
B | BLK | 1350 | Ground