For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel cluster. Refer to Instrument Cluster Replacement .
2. Remove the instrument panel cluster rear cover using a small flat bladed tool in order to release the retainer tabs.
3. Disconnect the required lamp from the cluster turning counterclockwise.
4. Remove the lamp from the cluster
5. Remove the bulb from the lamp socket, by pulling out.

### Installation Procedure

1. Install the bulb to the lamp socket pressing into place until fully seated.
2. Install the required lamp to the cluster.
3. Connect the required lamp to the cluster turning clockwise.
4. Install the instrument panel cluster rear cover pressing into place until fully seated.
5. Install the instrument panel cluster. Refer to Instrument Cluster Replacement .