For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Intermediate Shaft Lower Pinch Bolt | 22 N·m | 16 lb ft
Power Steering Hose Retainer Nut | 5 N·m | 45 lb in
Power Steering Pump Mounting Bolts (2.4L) | 26 N·m | 19 lb ft
Power Steering Pump Mounting Bolts (3.4L) | 34 N·m | 25 lb ft
Power Steering Pressure Hose Fitting | 27 N·m | 20 lb ft
Power Steering Return Hose Support Nut | 5 N·m | 45 lb in
Power Steering Return Pipe Fitting | 27 N·m | 20 lb ft
Steering Gear Bolts | 120 N·m | 89 lb ft
Tie Rod Jam Nut | 68 N·m | 50 lb ft
Tie Rod Nut | 45 N·m | 33 lb ft