For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Cable Bracket Bolts | 10 N·m | 89 lb in
Accelerator Pedal Nuts | 30 N·m | 22 lb ft
Air Cleaner Intake Duct Nut | 10 N·m | 89 lb in
Air Cleaner Intake Duct Screw | 10 N·m | 89 lb in
Air Cleaner Outlet Resonator Clamp | 5 N·m | 44 lb in
Air Cleaner Outlet Resonator Mounting Screws | 10 N·m | 89 lb in
CKP Sensor Bolts | 10 N·m | 89 lb in
CMP Sensor Bolts | 15 N·m | 11 lb ft
Engine Coolant Sensor | 20 N·m | 15 lb ft
EVAP Canister Purge Valve Mounting Bracket Nut | 8 N·m | 71 lb in
EVAP Canister Retainer Bolt | 10 N·m | 89 lb in
Exhaust Heat Shield Bolt | 2.0 N·m | 18 lb in
Exhaust Heat Shield Nut | 1.0 N·m | 9 lb in
Fuel Feed Pipe to Fuel Rail | 33 N·m | 24 lb ft
Fuel Filler Hose Clamp | 3 N·m | 27 lb in
Fuel Filter Fitting | 27 N·m | 20 lb ft
Fuel Pipe Mounting Bolts | 6 N·m | 53 lb in
Fuel Pipe Retainer Bolts | 12 N·m | 106 lb in
Fuel Pressure Regulator Attaching Screw | 9.5 N·m | 84 lb in
Fuel Rail Attaching Bolts | 26 N·m | 19 lb ft
Fuel Return Pipe Bracket Screw | 9.5 N·m | 84 lb in
Fuel Tank Retaining Strap Bolt | 35 N·m | 26 lb ft
HO2S 2 | 41 N·m | 30 lb ft
ICM Cover Bolts | 22 N·m | 16 lb ft
ICM Screws | 4 N·m | 35 lb in
Idle Air Control Valve | 3 N·m | 27 lb in
Ignition Coil Housing Screws | 4 N·m | 35 lb in
Knock Sensor | 25 N·m | 18 lb ft
MAP Sensor Attaching Screw | 6.5 N·m | 5.7 lb ft
MAP Sensor Bracket Bolt | 10 N·m | 89 lb in
O2S 1 | 41 N·m | 30 lb ft
PCM Electrical Connector Screws | 8 N·m | 71 lb in
Throttle Body Attaching Bolts | 10 N·m | 89 lb in
TP Sensor Mounting Screws | 2 N·m | 18 lb in
Upper Air Cleaner Cover Screws | 3 N·m | 26 lb in