For 1990-2009 cars

Table 1: | C101
Table 2: | C102, Automatic Transaxle
Table 3: | C130 (LA1 Only)
Table 4: | C200
Table 5: | C206
Table 6: | C207
Table 7: | C300
Table 8: | C301
Table 9: | C306
Table 10: | C400
Table 11: | C411
Table 12: | C412
Table 13: | C413 (Wheel Speed Sensors (WSS))
Table 14: | C413 (Canister Vent)
Table 15: | C413 (Fuel Systems)
Table 16: | C500
Table 17: | C501
Table 18: | C600
Table 19: | C700 (-A31)
Table 20: | C700 (A31)
Table 21: | C800 (w/A31)
Table 22: | C800 (-A31)

#### C101

Connector Part Information |

• | 12177081

• | 10-Way F Global Terminal 150 Series Sealed (BLK)

Connector Part Information

• | 12045808

• | 10-Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | DK GRN/WHT | 817 | VSS Signal | B | DK GRN/WHT | 817 | VSS Signal
C | GRY/BLK | 87 | Resume/Accel Switch Signal | C | GRY/BLK | 87 | Resume/Accel Switch Signal
D | DK BLU | 84 | Set/Coast Switch Signal | D | DK BLU | 84 | Set/Coast Switch Signal
E | RED | 228 | Windshield Washer Pump Control | E | RED | 228 | Windshield Washer Pump Control
F | BLK/WHT | 99 | Windshield Washer Fluid Level Signal | F | BLK/WHT | 99 | Windshield Washer Fluid Level Signal
G | YEL/BLK | 68 | Low Coolant Level Indicator Control | G | YEL/BLK | 68 | Low Coolant Level Indicator Control
H | GRY | 397 | Cruise Control On Switch Signal | H | GRY | 397 | Cruise Control On Switch Signal
J-K | -- | -- | Not Used | J-K | -- | -- | Not Used

#### C102, Automatic Transaxle

Connector Part Information |

• | 12160493

• | 20-Way F Micro-Pack 100 Series (GRY)

Connector Part Information

• | 12160782

• | 20-Way M Micro-Pack 100 Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | LT GRN | 1222 | (1-2 Shift Solenoid) Valve Control | A | LT GRN | 1222 | (1-2 Shift Solenoid) Valve Control
B | YEL/BLK | 1223 | (2-3 Shift Solenoid) Valve Control | B | YEL | 1223 | (2-3 Shift Solenoid) Valve Control
C | RED/BLK | 1228 | PC Solenoid Valve High Control (Sol A.) | C | PPL | 1228 | PC Solenoid Valve High Control (Sol A.)
D | LT BLU/WHT | 1229 | PC Solenoid Valve Low Control (Sol A.) | D | LT BLU | 1229 | PC Solenoid Valve Low Control (Sol A.)
E | PNK | 1039 | Ignition 1 Voltage | E | RED | 839 | Ignition 1 Voltage
F-K | -- | -- | Not Used | F-K | -- | -- | Not Used
L | YEL/BLK | 1227 | TFT Sensor Signal | L | BRN | 1227 | TFT Sensor Signal
M | WHT/BLK | 2762 | Low Reference | M | GRY | 452 | Low Reference
N | PNK | 1224 | Transmission Fluid Pressure Switch Signal A | N | PNK | 1224 | Transmission Fluid Pressure Switch Signal A
P | RED | 1226 | Transmission Fluid Pressure Switch Signal C | P | ORN | 1226 | Transmission Fluid Pressure Switch Signal C
R | DK BLU | 1225 | Transmission Fluid Pressure Switch Signal B | R | DK BLU | 1225 | Transmission Fluid Pressure Switch Signal B
S | RED/BLK | 1230 | AT ISS High Signal | S | BLK | 1230 | AT ISS High Signal
T | BRN | 418 | TCC PWM Solenoid Valve Control | T | TAN | 418 | TCC PWM Solenoid Valve Control
U | YEL | 657 | TCC Release Switch Signal | U | WHT | 1804 | TCC Release Switch Signal
V | DK BLU/WHT | 1231 | AT ISS Low Signal | V | DK GRN | 1231 | AT ISS Low Signal
W | -- | -- | Not Used | W | -- | -- | Not Used

#### C130 (LA1 Only)

Connector Part Information |

• | 15326084

• | 16-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 15326085

• | 16-Way M Metri-Pack Mixed Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PNK | 839 | Ignition 1 Voltage | A | PNK | 639 | Ignition 1 Voltage
B | YEL | 410 | ECT Sensor Signal | B | YEL | 410 | ECT Sensor Signal
C | BLK | 1744 | Fuel Injector 1 Control | C | BLK | 1744 | Fuel Injector 1 Control
D | LT GRN/BLK | 1745 | Fuel Injector 2 Control | D | LT GRN/BLK | 1745 | Fuel Injector 2 Control
E | PNK/BLK | 1746 | Fuel Injector 3 Control | E | PNK/BLK | 1746 | Fuel Injector 3 Control
F | LT BLU/BLK | 844 | Fuel Injector 4 Control | F | LT BLU/BLK | 844 | Fuel Injector 4 Control
G | BLK/WHT | 845 | Fuel Injector 5 Control | G | BLK/WHT | 845 | Fuel Injector 5 Control
H | YEL/BLK | 846 | Fuel Injector 6 Control | H | YEL/BLK | 846 | Fuel Injector 6 Control
J | -- | -- | Not Used | J | -- | -- | Not Used
K | BRN | 2704 | 5 Volt Reference | K | GRY | 2704 | 5 Volt Reference
L | ORN/BLK | 469 | Low Reference | L | ORN/BLK | 469 | Low Reference
M | LT GRN | 432 | MAP Sensor Signal | M | LT GRN | 432 | MAP Sensor Signal
N | RED/WHT | 812 | 12 Volt Reference | N | RED/WHT | 812 | 12 Volt Reference
P | BLK | 407 | Low Reference | P | BLK | 407 | Low Reference
R | BRN/WHT | 633 | CMP Sensor Signal | R | BRN/WHT | 633 | CMP Sensor Signal
S | -- | -- | Not Used | S | -- | -- | Not Used

#### C200

Connector Part Information |

• | 15304692

• | 18-Way F Global Terminal Mixed Series (BLK)

Connector Part Information

• | 15336468

• | 18-Way M Global Terminal Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | PPL | 1807 | Class 2 Serial Data (Primary) | A1 | PPL | 1807 | Class 2 Serial Data (Primary)
A2-A3 | -- | -- | Not Used | A2-A3 | -- | -- | Not Used
A4 | BLK | 250 | Ground | A4 | BLK | 250 | Ground
A5-A6 | -- | -- | Not Used | A5-A6 | -- | -- | Not Used
A7 | ORN/BLK | 556 | Low Reference | A7 | ORN/BLK | 556 | Low Reference
A8 | GRY | 1056 | Steering Wheel Position Sensor 5V Reference Voltage | A8 | GRY | 1056 | Steering Wheel Position Sensor 5V Reference Voltage
A9 | LT BLU | 1059 | Steering Wheel Position Sensor Signal | A9 | LT BLU | 1059 | Steering Wheel Position Sensor Signal
B1 | -- | 379 | CPP Switch Signal | B1 | -- | 379 | CPP Switch Signal
B2 | BLK/WHT | 451 | Ground | B2 | BLK/WHT | 451 | Ground
B3 | DK GRN/WHT | 817 | VSS Signal | B3 | DK GRN/WHT | 817 | VSS Signal
B4 | -- | -- | Not Used | B4 | -- | -- | Not Used
B5 | LT GRN | 24 | Backup Lamp Supply Voltage | B5 | LT GRN | 24 | Backup Lamp Supply Voltage
B6 | -- | -- | Not Used | B6 | -- | -- | Not Used
B7 | PPL | 1807 | Class 2 Serial Data (Primary) | B7 | PPL | 1807 | Class 2 Serial Data (Primary)
B8 | BRN/WHT | 419 | MIL Control | B8 | BRN/WHT | 419 | MIL Control
B9 | PPL | 1500 | Ignition 0 Voltage | B9 | PPL | 1500 | Ignition 0 Voltage

#### C206

Connector Part Information |

• | 12047886

• | 8-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12084256

• | 8-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 441 | Ignition 3 Voltage | A | BRN | 441 | Ignition 3 Voltage
B | DK BLU | 84 | Cruise Control Set/Coast Switch Signal | B | DK BLU | 84 | Cruise Control Set/Coast Switch Signal
C | GRY/BLK | 87 | Cruise Control Resume/Accel Switch Signal | C | GRY/BLK | 87 | Cruise Control Resume/Accel Switch Signal
D | GRY | 397 | Cruise Control On Switch Signal | D | GRY | 397 | Cruise Control On Switch Signal
E | BRN | 1244 | Instrument Panel Lamp Supply Voltage - 2 | E | BRN | 1244 | Instrument Panel Lamp Supply Voltage - 2
F | BLK | 150 | Ground | F | BLK | 150 | Ground
G | PNK | 314 | Radio On Signal (Pontiac) | G | PNK | 314 | Radio On Signal (Pontiac)
H | LT GRN | 1011 | Remote Radio Control Signal | H | LT GRN | 1011 | Remote Radio Control Signal

#### C207

Connector Part Information |

• | 12047886

• | 8-Way F Metri-Pack 150 Series (BLK)

Connector Part Information

• | 12084256

• | 8-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 441 | Ignition 3 Voltage | A | BRN | 441 | Ignition 3 Voltage
B | DK BLU | 84 | Cruise Control Set/Coast Switch Signal | B | DK BLU | 84 | Cruise Control Set/Coast Switch Signal
C | GRY/BLK | 87 | Cruise Control Resume/Accel Switch Signal | C | GRY/BLK | 87 | Cruise Control Resume/Accel Switch Signal
D | GRY | 397 | Cruise Control On Switch Signal | D | GRY | 397 | Cruise Control On Switch Signal
E | BRN | 1244 | Instrument Panel Lamp Supply Voltage - 2 | E | BRN | 1244 | Instrument Panel Lamp Supply Voltage - 2
F | BLK | 150 | Ground | F | BLK | 150 | Ground
G | -- | -- | -- | G | PNK | 314 | Radio On Signal (Pontiac)
H | LT GRN | 1011 | Remote Radio Control Signal | H | LT GRN | 1011 | Remote Radio Control Signal

#### C300

Connector Part Information |

• | 12064769

• | 10-Way F Metri-Pack 150 Series (NAT)

Connector Part Information

• | 12078169

• | 10-Way M Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BRN | 882 | Right Rear Wheel Speed Sensor Signal | A | BRN | 882 | Right Rear Wheel Speed Sensor Signal
B | WHT | 883 | Right Rear Wheel Speed Sensor Low Reference | B | WHT | 883 | Right Rear Wheel Speed Sensor Low Reference
C | BLK | 884 | Left Rear Wheel Speed Sensor Signal | C | BLK | 884 | Left Rear Wheel Speed Sensor Low Reference
D | RED | 885 | Left Rear Wheel Speed Sensor Low Reference | D | RED | 885 | Left Rear Wheel Speed Sensor Low Reference
E | BLK | 2759 | Low Reference | E | BLK | 2759 | Low Reference
F | GRY | 2709 | 5 Volt Reference | F | GRY | 2709 | 5 Volt Reference
G | DK GRN | 890 | Fuel Tank Pressure Sensor Signal | G | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
H | LT GRN | 275 | Neutral Safety Switch Park Signal | H | LT GRN | 275 | Neutral Safety Switch Park Signal
J | PPL | 1589 | Fuel Level Sensor Signal (-Primary) | J | PPL | 1589 | Fuel Level Sensor Signal (-Primary)
K | WHT | 1310 | EVAP Canister Vent Solenoid Control | K | WHT | 1310 | EVAP Canister Vent Solenoid Control

#### C301

Connector Part Information |

• | 12020397

• | 3-Way F Metri-Pack 280 Series (BLK)

Connector Part Information

• | 12124067

• | 3-Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PNK | 541 | Ignition 3 Voltage | A | BRN | 541 | Ignition 3 Voltage
B | -- | -- | Not Used | B | -- | -- | Not Used
C | BLK | 750 | Ground | C | BLK | 750 | Ground

#### C306

Connector Part Information |

• | 12064749

• | 2-Way F Metri-Pack 480 Series (BLK)

Connector Part Information

• | 12064750

• | 2-Way M Metri-Pack 480 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 540 | Battery Positive Voltage | A | ORN | 540 | Battery Positive Voltage
B | BLK | 550 | Ground | B | BLK | 550 | Ground

#### C400

Connector Part Information |

• | 12015416

• | 8-Way F Metri-Pack 280 Series (NAT)

Connector Part Information

• | 12186074

• | 8-Way M Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | ORN | 1732 | Courtesy Lamps Supply Voltage | A | ORN | 1732 | Courtesy Lamps Supply Voltage
A | BLK/WHT | 1732 | Courtesy Lamps Supply Voltage (W/Y71 and Y72) | A | -- | -- | --
B-C | -- | -- | Not Used | B-C | -- | -- | Not Used
D | BRN | 541 | Ignition 3 Voltage (w/Y71) | D | BRN | 541 | Ignition 3 Voltage (w/power mirrors)
E | WHT | 156 | Courtesy Lamp Low Control | E | WHT | 156 | Courtesy Lamp Low Control
E | BLK | 156 | Courtesy Low Control (w/Y71 and Y72) | E | -- | -- | --
F | -- | -- | Not Used | F | -- | -- | Not Used
G | BLK | 750 | Ground (w/Y71) | G | BLK | 750 | Ground (w/power mirrors)
H | BLK | 750 | Ground | H | BLK | 750 | Ground
H | BLK | 750 | Ground (w/Y71 and Y72) | H | -- | -- | --

#### C411

Connector Part Information |

• | 12168477

• | 4-Way F Metri-Pack 150 Series

Connector Part Information

• | 12176898

• | 4-Way M Metri-Pack 150 Series Insert Molded (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PPL | 30 | Fuel Level Sensor Signal | A | PPL | 30 | Fuel Level Sensor Signal
B | GRY | 120 | Fuel Pump Supply Voltage | B | GRY | 120 | Fuel Pump Supply Voltage
C | BLK | 150 | Ground | C | BLK | 150 | Ground
D | PPL | 30 | Fuel Level Sensor Signal | D | PPL | 30 | Fuel Level Sensor Signal

#### C412

Connector Part Information |

• | 12160482

• | 4-Way F Metri-Pack 150 Series

Connector Part Information

• | 12176898

• | 4-Way M Metri-Pack 150 Series Insert Molded (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | PPL | 30 | Fuel Level Sensor Signal | A | PPL | 30 | Fuel Level Sensor Signal
B | GRY | 120 | Fuel Pump Supply Voltage | B | GRY | 120 | Fuel Pump Supply Voltage
C | BLK | 150 | Ground | C | BLK | 150 | Ground
D | BLK/WHT | 30 | Fuel Level Sensor Signal | D | BLK/WHT | 30 | Fuel Level Sensor Signal

#### C413 (Wheel Speed Sensors (WSS))

Connector Part Information |

• | 12146439

• | 4-Way F Metri-Pack 150 Series Sealed (GRY)

Connector Part Information

• | 15326715

• | 16-Way M Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | WHT | 883 | Right Rear Wheel Speed Sensor Low Reference | 1A | WHT | 883 | Right Rear Wheel Speed Sensor Low Reference
B | BRN | 882 | Right Rear Wheel Speed Sensor Signal | 1B | BRN | 882 | Right Rear Wheel Speed Sensor Signal
C | RED | 885 | Left Rear Wheel Speed Sensor Low Reference | 1C | RED | 885 | Left Rear Wheel Speed Sensor Low Reference
D | BLK | 884 | Left Rear Wheel Speed Sensor Signal | 1D | BLK | 884 | Left Rear Wheel Speed Sensor Signal

#### C413 (Canister Vent)

Connector Part Information |

• | 15324263

• | 4-Way F Metri-Pack 150 Series Sealed (NAT)

Connector Part Information

• | 15326715

• | 16-Way M Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
A | BRN | 241 | Ignition 3 Voltage | 2A | BRN | 241 | Ignition 3 Voltage
B | WHT | 1310 | EVAP Canister Vent Solenoid Control | 2B | WHT | 1310 | EVAP Canister Vent Solenoid Control
C-D | -- | -- | Not Used | 2C-2D | -- | -- | Not Used

#### C413 (Fuel Systems)

Connector Part Information |

• | 15317611

• | 7-Way F Metri-Pack 280 Series (LT GRY)

Connector Part Information

• | 15326715

• | 16-Way M Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | BLK | 150 | Ground | 3A | BLK | 650 | Ground
B | BLK/WHT | 651 | Ground | 3B | BLK | 2759 | Low reference
C | GRY | 120 | Fuel Pump Supply Voltage | 3C | GRY | 120 | Fuel Pump Supply Voltage
D | PPL | 30 | Fuel Level Sensor Signal | 3D | PPL | 1589 | Fuel Level Sensor Signal (-Primary)
E | -- | -- | Not Used | 3E | -- | -- | Not Used
F | GRY/BLK | 416 | 5 Volt Reference | 3F | GRY | 2709 | 5 Volt Reference
G | DK GRN | 890 | Fuel Tank Pressure Sensor Signal | 3G | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
H | ORN/BLK | 469 | Low Reference | 3H | BLK | 2759 | Low Reference
H | -- | -- | -- | 3H | BLK | 2759 | Low Reference

#### C500

Connector Part Information |

• | 15304690

• | 18-Way F Global Terminal Mixed Series (GRY)

Connector Part Information

• | 15336467

• | 18-Way M Global Terminal Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | PPL/WHT | 889 | Right Mirror Motor Down (Oldsmobile) | A1 | PPL/WHT | 889 | Right Rear Motor Down (Oldsmobile)
A1 | BRN/WHT | 1498 | Right Rear Motor Up (Pontiac) | A1 | BRN/WHT | 1498 | Right Rear Motor Up (Pontiac)
A2 | RED/WHT | 881 | Right Mirror Motor Right | A2 | RED/WHT | 881 | Right Mirror Motor Right
A3 | -- | -- | Not Used | A3 | -- | -- | Not Used
A4 | LT BLU | 166 | Power Window Master Switch Right Front Up Signal | A4 | LT BLU | 166 | Power Window Master Switch Right Front Up Signal
A5 | TAN | 167 | Power Window Master Switch Right Front Down Signal | A5 | TAN | 167 | Power Window Master Switch Right Front Down Signal
A6 | BLK | 550 | Ground | A6 | BLK | 550 | Ground
A7-A9 | -- | -- | Not Used | A7-A9 | -- | -- | Not Used
B1 | GRY | 8 | Instrument Panel Lamp Supply Voltage -1 (Oldsmobile) | B1 | GRY | 8 | Instrument Panel Lamp Supply Voltage -1 (Oldsmobile)
B1 | -- | -- | Not Used (Pontiac) | B1 | -- | -- | Not Used (Pontiac)
B2 | BLK | 550 | Ground | B2 | BLK | 550 | Ground
B3 | -- | -- | Not Used | B3 | -- | -- | Not Used
B4 | BRN | 141 | Ignition 3 Voltage | B4 | BRN | 141 | Ignition 3 Voltage
B5 | YEL | 1956 | Left Front Tweeter Speaker Output (-) (w/U85) | B5 | YEL | 1956 | Left Front Tweeter Speaker Output (-) (w/U85)
B5 | -- | -- | Not Used (-U85) | B5 | -- | -- | Not Used (-U85)
B6 | BLK | 1856 | Left Front Tweeter Speaker Output (+) (w/U85) | B6 | BLK | 1856 | Left Front Tweeter Speaker Output (+) (w/U85)
B6 | -- | -- | Not Used (-U85) | B6 | -- | -- | Not Used (-U85)
B7 | -- | -- | Not Used | B7 | -- | -- | Not Used
B8 | ORN | 1840 | Battery Positive Voltage | B8 | ORN | 1840 | Battery Positive Voltage
B9 | GRY | 90 | Right Mirror Motor Left | B9 | GRY | 90 | Right Mirror Motor Left

#### C501

Connector Part Information |

• | 15304692

• | 18-Way F Global Terminal Mixed Series (BLK)

Connector Part Information

• | 15336468

• | 18-Way M Global Terminal Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | LT GRN/BLK | 394 | Left Front Door Handle Switch Signal | A1 | LT GRN/BLK | 394 | Left Front Door Handle Switch Signal
A2 | BLK/WHT | 1576 | Trunk Release Switch Signal | A2 | BLK | 1576 | Trunk Release Switch Signal
A3 | BLK | 550 | Ground | A3 | BLK | 550 | Ground
A4 | LT GRN | 170 | Power Window Master Switch Right Rear Up Signal (w/A31) | A4 | LT GRN | 170 | Power Window Master Switch Right Rear Up Signal (w/A31)
A5 | PPL | 171 | Power Window Master Switch Right Rear Down Signal (w/A31) | A5 | PPL | 171 | Power Window Master Switch Right Rear Down Signal
A6-A7 | -- | -- | Not Used | A6-A7 | -- | -- | Not Used
A8 | TAN | 294 | Driver Door Lock Motor Unlock | A8 | TAN | 694 | Door Lock Motor Unlock
A9 | GRY | 295 | Door Lock Motor Lock | A9 | GRY | 295 | Door Lock Motor Lock
B1 | GRY | 118 | Left Front Speaker Output (-) (-U85) | B1 | GRY | 118 | Left Front Speaker Output (-) (-U85)
B1 | LT BLU | 1957 | Left Front Midrange Speaker Output (-) (w/U85) | B1 | LT BLU | 1957 | Left Front Midrange Speaker Output (-) (w/U85)
B2 | BLK | 650 | Ground | B2 | BLK | 650 | Ground
B3 | WHT | 682 | Door Lock Lock/Unlock Signal | B3 | WHT | 682 | Door Lock Lock/Unlock Signal
B4 | DK BLU | 1307 | Power Window Master Switch Lockout Signal (w/A31) (Sedan) | B4 | DK BLU | 1307 | Power Window Master Switch Lockout Signal (Sedan)
B4-B6 | -- | -- | Not Used (Coupe) | B4-B6 | -- | -- | Not Used (Coupe)
B5 | DK GRN | 168 | Power Window Master Switch Left Rear Up Signal (Sedan) | B5 | DK GRN | 168 | Power Window Master Switch Left Rear Up Signal
B6 | PPL/WHT | 169 | Power Window Master Switch Left Rear Down Signal | B6 | PPL/WHT | 169 | Power Window Master Switch Left Rear Down Signal
B7 | GRY | 8 | Instrument Panel Lamp Supply Voltage -1 | B7 | GRY | 8 | Instrument Panel Lamp Supply Voltage -1
B8 | TAN | 201 | Left Front Speaker Output (+)(-U85) | B8 | TAN | 201 | Left Front Speaker Output (+)(-U85)
B8 | DK BLU | 1857 | Left Front Midrange Speaker Output (+)(w/U85) | B8 | DK BLU | 1857 | Left Front Midrange Speaker Output (+)(w/U85)
B9 | -- | -- | Not Used | B9 | -- | -- | Not Used

#### C600

Connector Part Information |

• | 15304692

• | 18-Way F Global Terminal Mixed Series (BLK)

Connector Part Information

• | 15336468

• | 18-Way M Global Terminal Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A1 | BRN/WHT | 1498 | Right Mirror Motor Down (Oldsmobile) | A1 | PPL/WHT | 889 | Right Mirror Motor Down (Oldsmobile)
A1 | BRN/WHT | 1498 | Right Mirror Motor Up (Pontiac) | A1 | BRN/WHT | 1498 | Right Mirror Motor Up (Pontiac)
A2 | RED/WHT | 881 | Right Mirror Motor Right | A2 | RED/WHT | 881 | Right Mirror Motor Right
A3 | BLK | 550 | Ground | A3 | BLK | 550 | Ground
A4 | LT BLU | 166 | Power Window Master Switch Right Front Up Signal | A4 | LT BLU | 166 | Power Window Master Switch Right Front Up Signal
A5 | TAN | 167 | Power Window Master Switch Right Front Down Signal | A5 | TAN | 167 | Power Window Master Switch Right Front Down Signal
A6 | LT BLU | 395 | Right Front Door Handle Switch Signal | A6 | LT BLU | 395 | Right Front Door Handle Switch Signal
A7 | -- | -- | Not Used | A7 | -- | -- | Not Used
A8 | TAN | 294 | Door Lock Motor Unlock | A8 | TAN | 294 | Door Lock Motor Unlock
A9 | GRY | 295 | Door Lock Motor Lock | A9 | GRY | 295 | Door Lock Motor Lock
B1 | DK GRN | 117 | Right Front Speaker Output (-) | B1 | DK GRN | 117 | Right Front Speaker Output (-)
B1 | DK GRN | 1953 | Right Front Midrange Speaker Output (-) (w/U85) | B1 | DK GRN | 1953 | Right Front Midrange Speaker Output (-) (w/U85)
B2 | BLK | 650 | Ground | B2 | BLK | 650 | Ground
B3 | WHT | 682 | Door Lock Lock/Unlock Signal | B3 | WHT | 682 | Door Lock Lock/Unlock Signal
B4 | DK BLU | 1307 | Power Window Master Switch Lockout Signal | B4 | DK BLU | 1307 | Power Window Master Switch Lockout Signal
B4 | BRN | 141 | Ignition 3 Voltage | B4 | BRN | 141 | Ignition 3 Voltage
B5-B6 | -- | -- | Not Used | B5-B6 | -- | -- | Not Used
B7 | GRY | 8 | Instrument Panel Lamp Supply Voltage -1 | B7 | GRY | 8 | Instrument Panel Lamp Supply Voltage -1
B8 | ORN | 1853 | Right Front Midrange Speaker Output (+) (U85) | B8 | ORN | 1853 | Right Front Midrange Speaker Output (+) (U85)
B8 | LT GRN | 200 | Right Front Speaker Output (+) (-U85) | B8 | LT GRN | 200 | Right Front Speaker Output (+) (-U85)
B9 | GRY | 90 | Right Mirror Motor Left | B9 | GRY | 90 | Right Mirror Motor Left

#### C700 (-A31)

Connector Part Information |

• | 12191687

• | 2-Way F Global Terminal 150 Series Sealed (BLU)

Connector Part Information

• | 12191681

• | 2-Way M Global Terminal 150 Series Sealed (BLU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | GRY | 295 | Door Lock Motor Lock | B | GRY | 295 | Door Lock Motor Lock
C | -- | -- | Not Used | C | -- | -- | Not Used
D | TAN | 294 | Door Lock Motor Unlock | D | TAN | 294 | Door Lock Motor Unlock
E-H | -- | -- | Not Used | E-H | -- | -- | Not Used

#### C700 (A31)

Connector Part Information |

• | 12191689

• | 7-Way F Global Terminal Mixed Series (NAT)

Connector Part Information

• | 12191677

• | 7-Way M Global Terminal Mixed Series (Sealed) (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | GRY | 295 | Door Lock Motor Lock | B | GRY | 295 | Door Lock Motor Lock
C | PPL | 169 | Power Window Master Switch Left Rear Down Signal | C | PPL | 169 | Power Window Master Switch Left Rear Down Signal
D | TAN | 294 | Door Lock Motor Unlock | D | TAN | 294 | Door Lock Motor Unlock
E-F | -- | -- | Not Used | E-F | -- | -- | Not Used
G | DK GRN | 168 | Power Window Master Switch Right Rear Up Signal | G | LT GRN | 168 | Power Window Master Switch Right Rear Up Signal
H | DK BLU | 1307 | Power Window Master Switch Lockout Signal | H | DK BLU | 1307 | Power Window Master Switch Lockout Signal

#### C800 (w/A31)

Connector Part Information |

• | 12191689

• | 7-Way F Global Terminal Mixed Series (NAT)

Connector Part Information

• | 12191677

• | 7-Way M Global Terminal Mixed Series (Sealed) (NAT)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | GRY | 295 | Door Lock Motor Lock | B | GRY | 295 | Door Lock Motor Lock
C | PPL | 171 | Power Window Master Switch Left Rear Down Signal | C | PPL | 171 | Power Window Master Switch Left Rear Down Signal
D | TAN | 294 | Door Lock Motor Unlock | D | TAN | 294 | Door Lock Motor Unlock
E-F | -- | -- | Not Used | E-F | -- | -- | Not Used
G | LT GRN | 170 | Power Window Master Switch Right Rear Up Signal | G | LT GRN | 170 | Power Window Master Switch Right Rear Up Signal
H | DK BLU | 1307 | Power Window Master Switch Lockout Signal | H | DK BLU | 1307 | Power Window Master Switch Lockout Signal

#### C800 (-A31)

Connector Part Information |

• | 12191687

• | 2-Way F Global Terminal 150 Series Sealed (BLU)

Connector Part Information

• | 12191681

• | 2-Way M Global Terminal 150 Series Sealed (BLU)

Pin | Wire Color | Circuit No. | Function | Pin | Wire Color | Circuit No. | Function
--- | --- | --- | --- | --- | --- | --- | ---
A | -- | -- | Not Used | A | -- | -- | Not Used
B | GRY | 295 | Door Lock Motor Lock | B | GRY | 295 | Door Lock Motor Lock
C | -- | -- | Not Used | C | -- | -- | Not Used
D | TAN | 294 | Door Lock Motor Unlock | D | TAN | 294 | Door Lock Motor Unlock
E-H | -- | -- | Not Used | E-H | -- | -- | Not Used