For 1990-2009 cars

### Removal Procedure

1. Remove the front seats. Refer to Seat Replacement .
2. Remove the console trim plate. Refer to Console Trim Plate Replacement .
3. Remove the rear cupholder to access the rear retaining screws.
4. Remove the front retaining screws.
5. Remove the console.

### Installation Procedure

1. Install the console.
2. Install the front and rear retaining screws.
3. Install the rear cupholder.
4. Install the console trim plate. Refer to Console Trim Plate Replacement .
5. Install the front seats. Refer to Seat Replacement .