For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Radio/Audio System Diagnostic System Check? | -- | Go to Step 2 | Go to Diagnostic System Check - Radio/Audio System
2 | Use the J 39916-A in order to perform the motor speed test. Is the cassette motor speed correct? | -- | Go to Step 3 | Go to Step 4
3 | Use the J 39916-A in order to clean the cassette player. Did you complete the repair? | -- | Go to Step 5 | --
4 | Important:: Perform the set up procedure for the radio. Replace the radio. Refer to Radio Replacement . Did you complete the replacement? | -- | Go to Step 5 | --
5 | Operate the system in order to verify the repair. Did you correct the condition? | -- | System OK | Go to Step 2