For 1990-2009 cars

Component | Location | Locator View | Connector End View
--- | --- | --- | ---
Engine Coolant Level Switch | In the right side of the engine compartment | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Engine Coolant Temperature (ECT) Sensor | On the top rear of the engine (LD9) | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Engine Coolant Temperature (ECT) Sensor | On the top left of the engine (LA1) | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
LH Cooling Fan Motor | In the front of the engine compartment | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Powertrain Control Module (PCM) | Below the left side of the IP near the steering column (LA1) | Engine Controls Component Views in Engine Controls | Powertrain Control Module Connector End Views in Engine Controls
Powertrain Control Module (PCM) | Below the left side of the IP near the steering column (LD9) | Engine Controls Component Views in Engine Controls | Powertrain Control Module Connector End Views in Engine Controls
RH Cooling Fan Motor | In the front of the engine compartment | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Underhood Junction Block | In the left side of the engine compartment | Power and Grounding Component Views in Wiring Systems | --
C102 (20 cavity) | On the left side of the engine | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C120 (2 cavity) | On the top rear of the engine (LA1) | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C130 (10 cavity) | On the top rear of the engine (LA1) | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G103 | On the left side of the engine | Harness Routing Views in Wiring Systems | --
S105 | In the engine harness, approximately 15 cm (5.9 in) from P100, towards the PCM | -- | --
P100 | In the rear of the engine compartment | Harness Routing Views in Wiring Systems | --