For 1990-2009 cars

### Removal Procedure

1. Remove the fuel tank. Refer to Fuel Tank Replacement .
2. Disconnect the fuel tank pressure sensor connector.
3. Remove the fuel tank pressure sensor from the fuel sender.

### Installation Procedure

1. Install the fuel tank pressure sensor to the fuel sender.
2. Connect the fuel tank pressure sensor connector.
3. Install the fuel tank. Refer to Fuel Tank Replacement .