For 1990-2009 cars

Table 1: | Door Lock Motor, Left Front
Table 2: | Door Lock Switch, Left Front (Pontiac, Oldsmobile Level 1)
Table 3: | Door Lock Switch, Left Front (Oldsmobile Level 2)
Table 4: | Power Window Motor, Left Front
Table 5: | Power Window Switch C1, Left Front (Sedan)
Table 6: | Power Window Switch C2, Left Front (Sedan)
Table 7: | Power Window Switch, Left Front (Coupe)
Table 8: | Power Window Switch, Right Front (Coupe)
Table 9: | Mirror Motor, Left Side (Pontiac)
Table 10: | Mirror Motor, Left Side (Oldsmobile)
Table 11: | Mirror Motor, Right Side (Pontiac)
Table 12: | Mirror Motor, Right Side (Oldsmobile)
Table 13: | Door Lock Motor, Left Rear
Table 14: | Power Window Motor, Left Rear
Table 15: | Power Window Switch, Left Rear
Table 16: | Power Mirror Switch (Pontiac)
Table 17: | Power Mirror Switch (Oldsmobile)
Table 18: | Door Lock Motor, Right Front
Table 19: | Door Lock Switch, Right Front (Pontiac)
Table 20: | Power Window Motor, Right Front
Table 21: | Power Window Switch, Right Front (Sedan)
Table 22: | Door Lock Motor, Right Rear
Table 23: | Power Window Motor, Right Rear
Table 24: | Power Window Switch, Right Rear

#### Door Lock Motor, Left Front

Connector Part Information |

• | 15300027

• | 2-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 294 | Power Door Lock Motor Feed (UNLOCK)
B | GRY | 295 | Power Door Lock Motor Feed (LOCK)

#### Door Lock Switch, Left Front (Pontiac, Oldsmobile Level 1)

Connector Part Information |

• | 12160882

• | 6-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | GRY | 8 | IP Lamp Feed
D | BLK | 650 | Ground
E | -- | -- | Not Used
F | WHT | 682 | Power Door Lock Switch Output

#### Door Lock Switch, Left Front (Oldsmobile Level 2)

Connector Part Information |

• | 12186854

• | 6-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A,B | -- | -- | Not Used
C | BLK | 650 | Ground
D | -- | -- | Not Used
E | GRY | 8 | IP Lamp Feed
F | WHT | 682 | Power Door Lock Switch Signal

#### Power Window Motor, Left Front

Connector Part Information |

• | 12129487

• | 2-Way F Metri-Pack 280 Series (MD GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 164 | Power Window Motor Feed, Left Front (UP)
B | GRY | 1136 | Power Window Motor Feed, Left Front (DOWN)

#### Power Window Switch C1, Left Front (Sedan)

Connector Part Information |

• | 12052854

• | 7-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | IP Lamp Feed
B | BLK | 550 | Ground
C | TAN | 167 | Power Window Master Switch Output, Right Front (DOWN)
D | GRY | 1136 | Power Window Master Switch Output, Left Front (DOWN)
E | DK BLU | 164 | Power Window Motor Feed, Left Front (UP)
F | LT BLU | 166 | Power Window Master Switch Output, Right Front (UP)
G | BRN | 141 | Fuse Output, Ignition 3 (Type III Fuse)

#### Power Window Switch C2, Left Front (Sedan)

Connector Part Information |

• | 12041429

• | 5-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 1307 | Power Window Master Switch Output (Lockout)
B | PPL | 171 | Power Window Master Switch Output, Right Rear (DOWN)
C | PPL/WHT | 169 | Power Window Master Switch Output, Left Rear (DOWN)
D | DK GRN | 168 | Power Window Master Switch Output, Left Rear (UP)
E | LT GRN | 170 | Power Window Master Switch Output, Right Rear (UP)

#### Power Window Switch, Left Front (Coupe)

Connector Part Information |

• | 12052854

• | 7-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | IP Lamp Feed
B | BLK | 550 | Ground
C | TAN | 167 | Power Window Master Switch Output, Right Front (DOWN)
D | DK BLU | 164 | Power Window Motor Feed, Left Front (UP)
E | GRY | 1136 | Power Window Master Switch Output, Left Front (DOWN)
F | LT BLU | 166 | Power Window Master Switch Output, Right Front (UP)
G | BRN | 141 | Fuse Output, Ignition 3 (Type III Fuse)

#### Power Window Switch, Right Front (Coupe)

Connector Part Information |

• | 12064998

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 166 | Power Window Master Switch Output, Right Front (UP)
B | BRN | 141 | Fuse Output, Ignition 3 (Type III Fuse)
C | BLK | 550 | Ground
D | DK BLU | 666 | Power Window Motor Feed, Right Front (UP)
E | TAN | 167 | Power Window Master Switch Output, Right Front (DOWN)
F | -- | -- | Not Used
G | GRY | 8 | IP Lamp Feed
H | BRN | 667 | Power Window Motor Feed, Right Front (DOWN)

#### Mirror Motor, Left Side (Pontiac)

Connector Part Information |

• | 12048458

• | 3-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 82 | Power Mirror Motor Feed, Left Horizontal Motor (LEFT)
B | WHT | 81 | Power Mirror Motor Feed, Left Horizontal Motor (RIGHT)
C | YEL | 88 | Power Mirror Motor Feed, Left Vertical Motor (UP)

#### Mirror Motor, Left Side (Oldsmobile)

Connector Part Information |

• | 12048458

• | 3-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 82 | Power Mirror Motor Feed, Left Horizontal Motor (LEFT)
B | WHT | 81 | Power Mirror Motor Feed, Left Horizontal Motor (RIGHT)
C | LT GRN | 89 | Power Mirror Motor Feed, Left Vertical Motor (DOWN)

#### Mirror Motor, Right Side (Pontiac)

Connector Part Information |

• | 12048458

• | 3-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 90 | Power Mirror Motor Feed, Right Horizontal Motor (LEFT)
B | RED/WHT | 881 | Power Mirror Motor Feed, Right Horizontal Motor (RIGHT)
C | BRN/WHT | 1498 | Power Mirror Motor Feed, Right Vertical Motor (UP)

#### Mirror Motor, Right Side (Oldsmobile)

Connector Part Information |

• | 12048458

• | 3-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 90 | Power Mirror Motor Feed, Right Horizontal Motor (LEFT)
B | RED/WHT | 881 | Power Mirror Motor Feed, Right Horizontal Motor (RIGHT)
C | PPL/WHT | 889 | Power Mirror Motor Feed, Right Vertical Motor (DOWN)

#### Door Lock Motor, Left Rear

Connector Part Information |

• | 15300027

• | 2-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 294 | Power Door Lock Motor Feed (UNLOCK)
B | GRY | 295 | Power Door Lock Motor Feed (LOCK)

#### Power Window Motor, Left Rear

Connector Part Information |

• | 12129487

• | 2-Way F Metri-Pack 280 Series (MD GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 668 | Power Window Motor Feed, Left Rear (UP)
B | BRN | 669 | Power Window Motor Feed, Left Rear (DOWN)

#### Power Window Switch, Left Rear

Connector Part Information |

• | 12064998

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 170 | Power Window Master Switch Output, Right Rear (DOWN)
B | DK BLU | 1307 | Power Window Master Switch Output (Lockout) m
C | -- | -- | Not Used
D | DK BLU | 668 | Power Window Motor Feed, Left Rear (UP)
E | PPL | 171 | Power Window Master Switch Output, Right Rear (UP)
F | -- | -- | Not Used
G | -- | -- | Not Used
H | BRN | 669 | Power Window Motor Feed, Left Rear (DOWN)

#### Power Mirror Switch (Pontiac)

Connector Part Information |

• | 12047886

• | 8-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN/WHT | 1498 | Power Mirror Motor Feed, Right Vertical Motor (UP)
B | RED/WHT | 881 | Power Mirror Motor Feed, Right Horizontal Motor (RIGHT)
C | GRY | 90 | Power Mirror Motor Feed, Right Horizontal Motor (LEFT)
D | BLK | 550 | Ground
E | ORN | 1840 | Fuse Output, Battery (Type III Fuse)
F | WHT | 81 | Power Mirror Motor Feed, Left Horizontal Motor (RIGHT)
G | YEL | 88 | Power Mirror Motor Feed, Left Vertical Motor (UP)
H | LT BLU | 82 | Power Mirror Motor Feed, Left Horizontal Motor (LEFT)

#### Power Mirror Switch (Oldsmobile)

Connector Part Information |

• | 12064769

• | 10-Way F Metri-Pack 150 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | IP Lamp Feed
B | BLK | 550 | Ground
C | PPL/WHT | 889 | Power Mirror Motor Feed, Right Vertical Motor (DOWN)
D | GRY | 90 | Power Mirror Motor Feed, Right Horizontal Motor (LEFT)
E | LT BLU | 82 | Power Mirror Motor Feed, Left Horizontal Motor (LEFT)
F | RED/WHT | 881 | Power Mirror Motor Feed, Right Horizontal Motor (RIGHT)
G | ORN | 1840 | Fuse Output, Battery (Type III Fuse)
H | -- | -- | Not Used
J | WHT | 81 | Power Mirror Motor Feed, Left Horizontal Motor (RIGHT)
K | LT GRN | 89 | Power Mirror Motor Feed, Left Vertical Motor (DOWN)

#### Door Lock Motor, Right Front

Connector Part Information |

• | 15300027

• | 2-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 294 | Power Door Lock Motor Feed (UNLOCK)
B | GRY | 295 | Power Door Lock Motor Feed (LOCK)

#### Door Lock Switch, Right Front (Pontiac)

Connector Part Information |

• | 12160882

• | 6-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | GRY | 8 | IP Lamp Feed
D | BLK | 650 | Ground
E | -- | -- | Not Used
F | WHT | 682 | Power Door Lock Switch Output

#### Power Window Motor, Right Front

Connector Part Information |

• | 12129487

• | 2-Way F Metri-Pack 280 Series (MD GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 666 | Power Window Motor Feed, Right Front (UP)
B | BRN | 667 | Power Window Motor Feed, Right Front (DOWN)

#### Power Window Switch, Right Front (Sedan)

Connector Part Information |

• | 12064998

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 666 | Power Window Motor Feed, Right Front (UP)
B | DK BLU | 1307 | Power Window Master Switch Output (Lockout)
C | BLK | 550 | Ground
D | DK BLU | 666 | Power Window Motor Feed, Right Front (UP)
E | TAN | 167 | Power Window Master Switch Output, Right Front (DOWN)
F | -- | -- | Not Used
G | GRY | 8 | IP Lamp Feed
H | BRN | 667 | Power Window Motor Feed, Right Front (DOWN)

#### Door Lock Motor, Right Rear

Connector Part Information |

• | 15300027

• | 2-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 294 | Power Door Lock Motor Feed (UNLOCK)
B | GRY | 295 | Power Door Lock Motor Feed (LOCK)

#### Power Window Motor, Right Rear

Connector Part Information |

• | 12129487

• | 2-Way F Metri-Pack 280 Series (MD GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 668 | Power Window Motor Feed, Right Rear (UP)
B | BRN | 669 | Power Window Motor Feed, Right Rear (DOWN)

#### Power Window Switch, Right Rear

Connector Part Information |

• | 12064998

• | 8-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 170 | Power Window Master Switch Output, Right Rear (DOWN)
B | DK BLU | 1307 | Power Window Master Switch Output (Lockout)
C | -- | -- | Not Used
D | DK BLU | 668 | Power Window Motor Feed, Right Rear (UP)
E | PPL | 171 | Power Window Master Switch Output, Right Rear (UP)
F | -- | -- | Not Used
G | -- | -- | Not Used
H | BRN | 669 | Power Window Motor Feed, Right Rear (DOWN)