For 1990-2009 cars

Table 1: | Camshaft Position (CMP) Sensor
Table 2: | Crankshaft Position (CKP) Sensor A
Table 3: | Crankshaft Position (CKP) Sensor B
Table 4: | Engine Coolant Temperature (ECT) Sensor
Table 5: | Evaporative Emission (EVAP) Canister Purge Solenoid
Table 6: | Evaporative Emission (EVAP) Canister Vent Solenoid
Table 7: | Exhaust Gas Recirculation (EGR) Valve
Table 8: | Fuel Injector 1
Table 9: | Fuel Injector 2
Table 10: | Fuel Injector 3
Table 11: | Fuel Injector 4
Table 12: | Fuel Injector 5
Table 13: | Fuel Injector 6
Table 14: | Fuel Pump and Sender Assembly
Table 15: | Fuel Tank Pressure (FTP) Sensor
Table 16: | Heated Oxygen Sensor (HO2S) Sensor 1
Table 17: | Heated Oxygen Sensor (HO2S) Sensor 2
Table 18: | Idle Air Control (IAC) Valve
Table 19: | Ignition Control Module (ICM), C1
Table 20: | Ignition Control Module (ICM), C2
Table 21: | Ignition Control Module (ICM), C3
Table 22: | Intake Air Temperature (IAT) Sensor
Table 23: | Knock Sensor (KS)
Table 24: | Manifold Absolute Pressure (MAP) Sensor
Table 25: | Mass Air Flow (MAF) Sensor
Table 26: | Throttle Position (TP) Sensor

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | 15336065

• | 3-Way F Global Terminal 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN/WHT | 633 | CMP Sensor Signal
B | BLK | 407 | Low Reference
C | RED/WHT | 812 | 12 Volt Reference

#### Crankshaft Position (CKP) Sensor A

Connector Part Information |

• | 12110294

• | 3-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED/WHT | 812 | 12 Volt Reference
B | LT BLU/BLK | 647 | Medium Resolution Engine Speed Signal
C | BLK | 407 | Low Reference

#### Crankshaft Position (CKP) Sensor B

Connector Part Information |

• | 12162192

• | 2-Way F Metri-Pack 150.2 Series Sealed Pull-to-Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 573 | CKP Sensor B Signal
B | PPL | 574 | Low Reference

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | 12162192

• | 2-Way F Metri-Pack 150.2 Series Sealed Pull-to-Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | Low Reference
B | YEL | 410 | ECT Sensor Signal

#### Evaporative Emission (EVAP) Canister Purge Solenoid

Connector Part Information |

• | 12052643

• | 2-Way F Metri-Pack 150 Series Sealed (RED)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 241 | Ignition 3 Voltage
B | DK GRN/WHT | 428 | EVAP Canister Purge Solenoid Control

#### Evaporative Emission (EVAP) Canister Vent Solenoid

Connector Part Information |

• | 12059862

• | 2-Way F Metri-Pack 150 Series Sealed (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 241 | Ignition 3 Voltage
B | WHT | 1310 | EVAP Canister Vent Solenoid Control

#### Exhaust Gas Recirculation (EGR) Valve

Connector Part Information |

• | 15306556

• | 5-Way F Global Terminal 150 Pull-to-Seat Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 435 | EGR Solenoid Low Control
B | BLK | 2753 | Low Reference
C | BRN | 1456 | EGR Valve Position Signal
D | BRN/WHT | 2702 | 5 Volt Reference
E | RED | 1676 | EGR Solenoid High Control

#### Fuel Injector 1

Connector Part Information |

• | 15326180

• | 2-Way F Micro-Pack 64 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition 1 Voltage
B | BLK | 1744 | Fuel Injector 1 Control

#### Fuel Injector 2

Connector Part Information |

• | 15326180

• | 2-Way F Micro-Pack 64 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition 1 Voltage
B | LT GRN/BLK | 1745 | Fuel Injector 2 Control

#### Fuel Injector 3

Connector Part Information |

• | 15326180

• | 2-Way F Micro-Pack 64 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition 1 Voltage
B | PNK/BLK | 1746 | Fuel Injector 3 Control

#### Fuel Injector 4

Connector Part Information |

• | 15326180

• | 2-Way F Micro-Pack 64 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition 1 Voltage
B | LT BLU/BLK | 844 | Fuel Injector 4 Control

#### Fuel Injector 5

Connector Part Information |

• | 15326180

• | 2-Way F Micro-Pack 64 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition 1 Voltage
B | BLK/WHT | 845 | Fuel Injector 5 Control

#### Fuel Injector 6

Connector Part Information |

• | 15326180

• | 2-Way F Micro-Pack 64 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 639 | Ignition 1 Voltage
B | YEL/BLK | 846 | Fuel Injector 6 Control

#### Fuel Pump and Sender Assembly

Connector Part Information |

• | 12160482

• | 4-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 30 | Fuel Level Sensor Signal
B | GRY | 120 | Fuel Pump Supply Voltage
C | BLK | 150 | Ground
D | GRY | 651 | Ground

#### Fuel Tank Pressure (FTP) Sensor

Connector Part Information |

• | 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | Low Reference
B | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
C | GRY | 416 | 5 Volt Reference

#### Heated Oxygen Sensor (HO2S) Sensor 1

Connector Part Information |

• | 12176896

• | 4-Way F Metri-Pack 150 Series Sealed (LT GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 413 | Low Reference
B | PPL | 412 | HO2S High Signal Sensor 1
C | BLK/WHT | 3113 | HO2S Heater Low Control (Bank 1 Sensor 1)
D | BRN | 241 | Ignition 3 Voltage

#### Heated Oxygen Sensor (HO2S) Sensor 2

Connector Part Information |

• | 12160825

• | 4-Way M Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/WHT | 1669 | HO2S Low Signal (Bank 1 Sensor 2)
B | PPL/WHT | 1668 | HO2S High Signal (Bank 1 Sensor 2)
C | BLK | 250 | Ground
D | BRN | 241 | Ignition 3 Voltage

#### Idle Air Control (IAC) Valve

Connector Part Information |

• | 12162187

• | 4-Way F Metri-Pack 150.2 Series Pull-to-Seat Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/BLK | 444 | IAC Coil B Low Control
B | LT GRN/WHT | 1749 | IAC Coil B High Control
C | LT BLU/BLK | 1748 | IAC Coil A Low Control
D | LT BLU/WHT | 1747 | IAC Coil A High Control

#### Ignition Control Module (ICM), C1

Connector Part Information |

• | 12059220

• | 6-Way F Metri-Pack 150.1 Series Pull-to-Seat Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/BLK | 424 | IC Timing Signal
B | WHT | 423 | IC Timing Control
C-D | -- | -- | Not Used
E | PPL/WHT | 430 | Low Resolution Engine Speed Signal
F | RED/BLK | 453 | Low Reference

#### Ignition Control Module (ICM), C2

Connector Part Information |

• | 12065558

• | 3-Way F Metri-Pack 150 Series Pull-to-Seat Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 573 | CKP Sensor B Signal
B | -- | -- | Not Used
C | PPL | 574 | Low Reference

#### Ignition Control Module (ICM), C3

Connector Part Information |

• | 12162192

• | 2-Way F Metri-Pack 150.2 Series Pull-to-Seat Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 450 | Ground
B | PNK | 239 | Ignition 1 Voltage

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | 12162196

• | 2-Way F Metri-Pack 150.2 Series Pull-to-Seat Sealed (MD GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 2760 | Low Reference
B | TAN | 472 | IAT Sensor Signal

#### Knock Sensor (KS)

Connector Part Information |

• | 400309

• | 1-Way F Metri-Pack 150 Series Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | DK BLU | 496 | Knock Sensor Signal

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | 12020403

• | 3-Way M Weather Pack Sealed (DK GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | Low Reference
B | LT GRN | 432 | MAP Sensor Signal
C | GRY | 2704 | 5 Volt Reference

#### Mass Air Flow (MAF) Sensor

Connector Part Information |

• | 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 492 | MAF Sensor Signal
B | BLK/WHT | 451 | Ground
C | PNK | 639 | Ignition 1 Voltage

#### Throttle Position (TP) Sensor

Connector Part Information |

• | 12065286

• | 3-Way F Metri-Pack 150 Series Pull-to-Seat Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY/BLK | 2701 | 5 Volt Reference
B | BLK | 2752 | Low Reference
C | DK BLU | 417 | TP Sensor Signal