For 1990-2009 cars

Problem | Correction
--- | ---
DEFINITION: Adjuster will not unlock.

- The locking wire is too loose or is disconnected.

Tighten the locking wire enough in order to allow the following actions to occur simultaneously:

• | The lock control lever activates.

• | The lock bar disengages from the locking slots in the adjuster lower channel.

- The adjuster lock bar sticks or binds.

• | Lubricate the lock bar pivot.

• | Eliminate the cause of the binding. Replace the adjuster if the bar is binding.