For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Fascia to Front Support Bracket Screws | 6 N·m | 53 lb in
Fascia to Quarter Panel Screws | 6 N·m | 53 lb in
Filler Panel Nut | 3 N·m | 27 lb in
Front Fascia To Fender Bolts | 10 N·m | 89 lb in
Front Impact Bar Nuts | 27 N·m | 20 lb ft
Front Support Bracket Screws | 6 N·m | 53 lb in
Inside Fascia Bolt | 3 N·m | 27 lb in
Rear Fascia Reinforcement Nuts | 10 N·m | 89 lb in
Rear Impact Bar Retaining Nut | 25 N·m | 18 lb ft
Rear Support Bracket Bolts | 3 N·m | 27 lb in
Rear Support Bracket Nuts | 10 N·m | 89 lb in
Rear Support Bracket Screws | 3 N·m | 27 lb in